Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	05/08/91	Elevation:	470 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6163330 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	317470  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.8 m deep,Porous, Schist 
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	11 % 	Aspect:	130 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Um1.44
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, 0.26-0.5m, Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus camaldulensis
	Surface Coarse Fragments:	0-2%, stony, 200-600mm, angular, Schist
	Profile Morphology
	A11	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Silty loam; Weak grade of structure, <2 mm, Granular; 
	Rough-ped fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Very weak consistence; Field pH 6 (Raupach, 0.05); Many, very fine (0-1mm) 
	roots; 
	A11	0.1 - 0.3 m	; Silty loam; Moist; 2-10%, stony, 200-600mm, angular tabular, dispersedstrong, Schist, coarse 
	fragments; Field pH 6 (Raupach, 0.2); Many, very fine (0-1mm) roots; 
	A11	0.3 - 0.5 m	Very dark grey (10YR3/1-Moist); , 2-10% , Distinct; Silty loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Very weak consistence; Field pH 6 (Raupach, 0.4); Many, very fine (0-1mm) roots; 
	A12	0.5 - 0.7 m	Dark grey (10YR4/1-Moist); , 2-10% , Distinct; Silty loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Very weak consistence; Field pH 6 (Raupach, 0.6); Common, very fine (0-1mm) roots; Clear 
	change to - 
	A2	0.7 - 0.8 m	Brown (10YR5/3-Moist); ; Sand; Massive grade of structure; Sandy (grains prominent) fabric; 
	Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very 
	weak consistence; Few, very fine (0-1mm) roots; Clear change to - 
	C	0.8 - 0.9 m	Yellowish red (5YR5/8-Moist); , 10-20% , Distinct; Sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Very weak consistence; Field pH 6 (Raupach, 0.9); Few, very fine (0-1mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile