Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	05/08/91	Elevation:	522 metres
	Map Ref.:	Sheet No. : 6728-20   1:10000	Rainfall:	No Data
	Northing/Long.:	6163800 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	317960  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.8 m deep,Schist 
	Land Form
	Rel/Slope Class: 	Rolling low hills 30-90m 10-	Pattern Type:	Hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	160 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, Minor or present (wind); 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.81
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Loamy sand; Massive grade of structure; 
	Sandy (grains prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2)  macropores, 
	Moist; Very weak consistence; Field pH 6 (Raupach, 0.05); Many, very fine (0-1mm) roots; 
	A12	0.1 - 0.3 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2)  macropores, Moist; Very weak 
	consistence; Field pH 6 (Raupach, 0.2); Many, very fine (0-1mm) roots; 
	A12	0.3 - 0.5 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2)  macropores, Moist; Very weak 
	consistence; Field pH 5.5 (Raupach, 0.4); Many, very fine (0-1mm) roots; 
	A12	0.5 - 0.6 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Massive grade of structure; Earthy fabric; Fine, (0 -
	 5) mm crack; Many (>5 per 100mm2)  macropores, Moist; Very weak consistence; Field pH 5.5 
	(Raupach, 0.55); Common, very fine (0-1mm) roots; Clear change to - 
	B	0.6 - 0.75 m	Brownish yellow (10YR6/6-Moist); , 0-0% ; Sandy clay; Massive grade of structure; Earthy fabric; 
	Fine, (0 - 5) mm crack; Common (1-5 per 100mm2)  macropores, Moist; Firm consistence; Field 
	pH 6 (Raupach, 0.7); Few, very fine (0-1mm) roots; Abrupt change to - 
	C	0.75 - 1 m	Red (2.5YR4/8-Moist); , 2-10% , Distinct; Sand; Massive grade of structure; Earthy fabric; Fine, 
	(0 - 5) mm crack; Many (>5 per 100mm2)  macropores, Moderately moist; Very firm consistence; 
	Field pH 5.5 (Raupach, 0.92); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	280	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile