Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	300	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	08/08/91	Elevation:	436 metres
	Map Ref.:	Sheet No. : 6628-26   1:10000	Rainfall:	No Data
	Northing/Long.:	6151001 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	311935  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.5 m deep,Slightly porous, 
	Schist 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	2 % 	Aspect:	30 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy5.61
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Confidence level not specified	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - Spyridium parvifolium
	Mid Strata - Tree, 6.01-12m, . *Species includes - Acacia pycnantha
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus fastigata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR5/3-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy fabric; Fine, (0 - 
	5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very weak 
	consistence; Field pH 6 (Raupach, 0.05); Many, very fine (0-1mm) roots; Clear change to - 
	A2	0.1 - 0.3 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Wet; 
	Very weak consistence; Field pH 6 (Raupach, 0.2); Common, very fine (0-1mm) roots; Abrupt 
	change to - 
	Bt	0.3 - 0.5 m	Brownish yellow (10YR6/6-Moist); , 10-20% , Distinct; Medium clay; Massive grade of structure; 
	Earthy fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Firm consistence; Field pH 6 (Raupach, 0.35); Few, very fine (0-1mm) roots; Clear change
	 to - 
	Bt	0.5 - 0.7 m	Brownish yellow (10YR6/6-Moist); , 20-50% , Distinct; Medium clay; Massive grade of structure; 
	Earthy fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Firm consistence; 0-2%, coarse gravelly, 20-60mm, subrounded, dispersedstrong, Quartz,
	 coarse fragments; Field pH 6 (Raupach, 0.6); Few, very fine (0-1mm) roots; Clear change to - 
	Bt	0.7 - 1 m	White (10YR8/2-Moist); , 2-10% , Distinct; Medium clay; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Firm consistence; Field pH 6 (Raupach, 0.9); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	300	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	300	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile