Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	316	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	09/08/91	Elevation:	419 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6159480 AMG zone: 54	Runoff:	Very slow
	Easting/Lat.:	315170  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	3 m deep,No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	Flat	Relief:	9 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0.5 % 	Aspect:	120 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dd4.11
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Confidence level not specified	soil
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Silty loam; Moderate grade of structure, 2-5 mm, 
	Granular; Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm)
	 macropores, Moist; Field pH 5.5 (Raupach, 0.05); Many, very fine (0-1mm) roots; 
	A12	0.1 - 0.2 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Silty loam; Moderate grade of structure, 2-5 mm, 
	Granular; Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm)
	 macropores, Moist; Field pH 5.5 (Raupach, 0.15); Many, very fine (0-1mm) roots; 
	A12	0.2 - 0.3 m	Very dark grey (2.5Y3/0-Moist); , 0-0% ; Silty loam; Massive grade of structure; Earthy fabric; 
	Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Field pH 5.5 (Raupach, 0.25); Many, very fine (0-1mm) roots; 
	A12	0.3 - 0.5 m	Very dark grey (2.5Y3/0-Moist); , 0-2% , Faint; Silty loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Field pH 5.5 (Raupach, 0.4); Common, very fine (0-1mm) roots; 
	A12	0.5 - 0.8 m	Very dark grey (2.5Y3/0-Moist); , 0-2% , Faint; Silty loam; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Moist; Field pH 6.5 (Raupach, 0.65); Common, very fine (0-1mm) roots; Clear change to - 
	Bt	0.8 - 1 m	Very dark grey (2.5Y3/0-Moist); , 0-2% , Faint; Medium clay; Massive grade of structure; Earthy 
	fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Field pH 6.5 (Raupach, 0.95); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	316	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	316	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile