Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/03/92	Elevation:	418 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6157100 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	318850  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 3 m deep,No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Peneplain
	Morph. Type:	Open depression (vale)	Relief:	5 metres
	Elem. Type:	Drainage depression	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	310 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Sodosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.3 m	Light grey (10YR7/2-Moist); , 0-2% , Distinct; Loamy sand; Massive grade of structure; Very few 
	(0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Few, very fine (0-1mm) roots; Sharp, Tongued 
	change to - 
	Bt	0.3 - 0.5 m	Dark grey (5Y4/1-Moist); , 10-20% , Prominent; Heavy clay; Strong grade of structure, 50-100 mm,
	 Columnar; Rough-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-
	1mm) macropores, Moist; Strong consistence; Many cutans, >50% of ped faces or walls coated,
	 prominent; Few, very fine (0-1mm) roots; Clear, Irregular change to - 
	Bts	0.5 - 0.7 m	Yellowish brown (10YR5/8-Moist); , 20-50% , Prominent; Medium clay; Strong grade of structure,
	 20-50 mm, Prismatic; Rough-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Moist; Strong consistence; Many cutans, >50% of ped faces or walls 
	coated, distinct; Clear, Irregular change to - 
	Bts	0.7 - 1 m	Yellowish brown (10YR5/8-Moist); , 10-20% , Prominent; Heavy clay; Strong grade of structure, 
	20-50 mm, Angular blocky; Rough-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very 
	fine (0.075-1mm) macropores, Moist; Very firm consistence; Many cutans, >50% of ped faces or 
	walls coated, prominent; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Nodules; Clear,
	 Smooth change to - 
	Bts	1 - 1.2 m	Yellowish brown (10YR5/8-Moist); , 10-20% , Prominent; Medium clay; Moderate grade of 
	structure, 50-100 mm, Angular blocky; Rough-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Very firm consistence; Common cutans, 
	10-50% of ped faces or walls coated, prominent; Few (2 - 10 %), Calcareous, Coarse (6 - 20 
	mm), Nodules; Clear, Wavy change to - 
	Bcg	1.2 - 1.5 m	Yellowish brown (10YR5/8-Moist); , 10-20% , Prominent; Sandy clay; Moderate grade of 
	structure, 100-200 mm, Prismatic; Rough-ped fabric; Moist; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	403	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile