Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	11/03/92	Elevation:	440 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6154800 AMG zone: 54	Runoff:	Slow
	Easting/Lat.:	319250  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.4 m deep,Slightly porous, 
	Silcrete 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	310 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Hydrosol     	Principal Profile Form:	Dy5.81
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 20.01-35m, Sparse. *Species includes - Pinus radiata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	O	0 - 0.02 m	Organic Layer; Dark grey (10YR4/1-Moist); ; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) 
	Medium (2-5mm) macropores, Weak consistence; Field pH 5 (Raupach, 0.01); Many, very fine (0-
	1mm) roots; Sharp, Smooth change to - 
	A1	0.02 - 0.25 m	Brown (10YR5/3-Moist); , 10-20% , Faint; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Weak consistence; Field pH 5.5 (Raupach, 0.2); Many, fine (1-2mm) roots; 
	Clear, Smooth change to - 
	A2	0.25 - 0.35 m	White (10YR8/2-Moist); , 10-20% , Distinct; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Weak consistence; 10-20%, coarse gravelly, 20-60mm, angular, 
	stratifiedstrong, Quartz, coarse fragments; Field pH 6 (Raupach, 0.3); Few, very fine (0-1mm) 
	roots; Sharp, Smooth change to - 
	Bt	0.35 - 0.4 m	Brownish yellow (10YR6/6-Moist); , 10-20% , Distinct; Medium clay; Massive grade of structure; 
	Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, stratifiedstrong, 
	Quartz, coarse fragments; Field pH 6 (Raupach, 0.36); Few, very fine (0-1mm) roots; Sharp, 
	Smooth change to - 
	Bq	0.4 -  m	; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately 
	moist; Very strong consistence; Duripan, Very strongly cemented, Continuous, Massive; Field 
	pH 8 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	404	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile