Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	408	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	I. Hollingsworth	Locality:
	Date Desc.:	12/03/92	Elevation:	440 metres
	Map Ref.:	1:10000	Rainfall:	No Data
	Northing/Long.:	6154000 AMG zone: 54	Runoff:	Moderately rapid
	Easting/Lat.:	318250  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 0.6 m deep,Schist 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Hills
	10%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	310 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Stable, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Confidence level not specified	soil
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Closed or dense. *Species includes - Pinus radiata
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, rounded, Ironstone
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; Sandy loam; Strong grade of structure, 2-5 mm, Granular; Weak 
	grade of structure; Moderately moist; Very firm consistence; Many cutans, >50% of ped faces or 
	walls coated, distinct; Field pH 6 (Raupach, 0.05); Many, very fine (0-1mm) roots; Clear, Smooth 
	change to - 
	A2	0.1 - 0.2 m	Light grey (10YR7/2-Moist); , 0-0% ; Sand; Massive grade of structure; Dry; Weak consistence; 
	20-50%, medium gravelly, 6-20mm, rounded, stratifiedstrong, Quartz, coarse fragments; Field pH
	 6.5 (Raupach, 0.15); Few, very fine (0-1mm) roots; Sharp, Smooth change to - 
	Bw	0.2 - 0.3 m	Yellowish brown (10YR5/8-Moist); , 2-10% , Distinct; 20-50%, medium gravelly, 6-20mm, 
	rounded, stratifiedstrong, Eolian sand, coarse fragments; Field pH 7 (Raupach, 0.2); Few, very 
	fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	408	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Warren Reservoir Catchment Survey
	Project Code:	WRN	Site ID:	408	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile