Project Name:	Yudnapina Station, S.A.
	Project Code:	YS1	Site ID:	A135	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Site Information
	Desc. By:	E.A. Jackson	Locality:	WAITE GRAZING EXPT AREA P120
	Date Desc.:	22/09/54	Elevation:	 90 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	137.220277777778	Runoff:	Very slow
	Easting/Lat.:	-32.0580555555556	Drainage:	Very poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endohypersodic Epic Calcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Mid Strata - Chenopod shrub, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.06 m	Reddish yellow (5YR6/6-Moist); ; Sandy loam; Very weak consistence; , Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.06 - 0.23 m	Reddish yellow (5YR6/6-Moist); ; Sandy clay loam; Weak consistence; , Calcareous, , Soft 
	segregations; Diffuse change to - 
	0.23 - 0.46 m	Light red (2.5YR6/8-Moist); ; Clay loam; Firm consistence; , Calcareous, , Soft segregations; 
	Clear change to - 
	0.46 - 0.7 m	Light red (2.5YR6/8-Moist); ; Medium clay; Firm consistence; , Calcareous, , Soft segregations; 
	Clear change to - 
	0.7 - 0.89 m	Red (2.5YR5/8-Moist); ; Medium clay; Firm consistence; , Calcareous, , Soft segregations; 
	1.4 - 1.55 m	Red (2.5YR5/8-Moist); ; Medium clay; Very firm consistence; , Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	YUDNAPINNA STN

	Project Name:	Yudnapina Station, S.A.
	Project Code:	YS1	Site ID:	A135	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	8.7H	 0.037C	 9.5K	 2.8	 1.7	 0.32
	0.06 - 0.23	9H	 0.038C
	0.23 - 0.46	9.1H	 0.044C
	0.46 - 0.7	9.4H	 0.054C
	0.7 - 0.89	9.5H	 0.065C
	1.4 - 1.55	9.8H	 0.085C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 0.17C	 0.017F	 0.039B	 0.71B	 50C	 18	 9	 22
	0.06 - 0.23	 1.7C	 0.018F	 0.035B	 0.77B	 46C	 18	 9	 25
	0.23 - 0.46	 5.4C	 36C	 20	 6	 32
	0.46 - 0.7	 9C	 0.018F	 0.66B	 36C	 19	 2	 33
	0.7 - 0.89	 13C	 34C	 19	 1	 32
	1.4 - 1.55	 20C	<1	 34C	 18	 2	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06	 0.1B
	0.06 - 0.23	 0.1B
	0.23 - 0.46	 0.13B
	0.46 - 0.7
	0.7 - 0.89
	1.4 - 1.55

	Project Name:	Yudnapina Station, S.A.
	Project Code:	YS1	Site ID:	A135	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (SA)
	Laboratory Analyses Completed for this profile
	10A_NR	Total element - S(%) - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate