Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1105	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	B. Purdie	Locality:
	Date Desc.:	21/04/98	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6525524 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	412455  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion:	 (sheet)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Black Kandosol     	Principal Profile Form:	Gn1.11
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse 
	Profile 
	1A1	0 - 0.35 m	Very dark brown (10YR2/2-Moist); ; Loam; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Moderately moist; Firm consistence; Field pH 7 (pH meter); Many, medium (2-5mm) roots; Clear, 
	Smooth change to - 
	2B21w	0.35 - 0.55 m	Very dark greyish brown (10YR3/2-Moist); Mechanical, 7.5YR66, 2-10% , 0-5mm, Distinct; Clay loam, 
	sandy; Massive grade of structure; Moderately moist; Firm consistence; Field pH 7.1 (pH meter); 
	Common, medium (2-5mm) roots; Clear, Smooth change to - 
	3B22w	0.55 - 0.85 m	Dark greyish brown (10YR4/2-Moist); Mottles, 7.5YR46, 2-10% , 0-5mm, Faint; Fine sandy clay loam; 
	Massive grade of structure; Moderately moist; Firm consistence; 2-10%, coarse fragments; Field pH 6.7 
	(pH meter); Common, medium (2-5mm) roots; Clear, Smooth change to - 
	4B23w	0.85 - 1.1 m	Dark greyish brown (10YR4/2-Moist); Mottles, 7.5YR46, 10-20% , 0-5mm, Faint; Loam; Massive grade 
	of structure; Moist; Firm consistence; 2-10%, coarse fragments; Field pH 5.4 (pH meter); Common, 
	medium (2-5mm) roots; Clear, Smooth change to - 
	5B24w	1.1 - 1.6 m	Brown (10YR4/3-Moist); ; Sandy clay loam; Massive grade of structure; Moist; Firm consistence; 2-10%,
	 fine gravelly, 2-6mm, subangular, Gneiss, coarse fragments; Field pH 5.4 (pH meter); Few, medium (2-
	5mm) roots; 
	1.6 -  m	; Sandy clay loam; 
	Morphological Notes
	3B22w	Abundant mica flakes.
	4B23w	Sand lenses.
	5B24w	Gravely sand lenses.
	Observation Notes
	Site Notes
	Photos Rolls 58 - 9/10.  Deep yellow duplex over loam. Saline at 1m. Effective soil depth is less due to salinity.

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1105	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	5.6B	4B	12.47H	9.22	0.28	0.33	0.04J	22.3D
	6.6H
	0 - 0.14	5.6B	4B	12.47H	9.22	0.28	0.33	0.04J	22.3D
	6.6H
	0 - 0.14	5.6B	4B	12.47H	9.22	0.28	0.33	0.04J	22.3D
	6.6H
	0.07 - 0.12
	0.35 - 0.55	5.4B	4B	5.01A	6.05	0.3	0.46	11.82D
	6.7H
	0.35 - 0.55	5.4B	4B	5.01A	6.05	0.3	0.46	11.82D
	6.7H
	0.35 - 0.55	5.4B	4B	5.01A	6.05	0.3	0.46	11.82D
	6.7H
	0.38 - 0.43
	0.55 - 0.85	5.4B	13B	3.84H	4.32	0.16	0.53	0.05J	8.85D
	6.2H
	0.55 - 0.85	5.4B	13B	3.84H	4.32	0.16	0.53	0.05J	8.85D
	6.2H
	0.55 - 0.85	5.4B	13B	3.84H	4.32	0.16	0.53	0.05J	8.85D
	6.2H
	0.57 - 0.62
	0.85 - 1.1	5B	230B	4.09H	5.45	0.28	1.15	0.23J	10.97D
	5.3H
	0.85 - 1.1	5B	230B	4.09H	5.45	0.28	1.15	0.23J	10.97D
	5.3H
	0.85 - 1.1	5B	230B	4.09H	5.45	0.28	1.15	0.23J	10.97D
	5.3H
	1.1 - 1.5	5B	210B	1.79H	3.58	0.16	0.96	0.11J	6.49D
	5.4H
	1.1 - 1.5	5B	210B	1.79H	3.58	0.16	0.96	0.11J	6.49D
	5.4H
	1.1 - 1.5	5B	210B	1.79H	3.58	0.16	0.96	0.11J	6.49D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	4.47D	350B	0.274E	27.5	20.2
	0 - 0.14	4.47D	350B	0.274E	27.5	20.2
	0 - 0.14	4.47D	350B	0.274E	27.5	20.2
	0.07 - 0.12	0.80
	0.35 - 0.55	2.56D	300B	0.149E	21.1	23
	0.35 - 0.55	2.56D	300B	0.149E	21.1	23
	0.35 - 0.55	2.56D	300B	0.149E	21.1	23
	0.38 - 0.43	1.00
	0.55 - 0.85	1.28D	220B	0.07E	70.1I	11.6	18.3
	0.55 - 0.85	1.28D	220B	0.07E	70.1I	11.6	18.3
	0.55 - 0.85	1.28D	220B	0.07E	70.1I	11.6	18.3
	0.57 - 0.62	1.20
	0.85 - 1.1	2.02D	250B	0.098E	66.3I	13.8	19.9

	Project Name:	Chittering land resources survey
	Project Code:	CHT	Site ID:	1105	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.85 - 1.1	2.02D	250B	0.098E	66.3I	13.8	19.9
	0.85 - 1.1	2.02D	250B	0.098E	66.3I	13.8	19.9
	1.1 - 1.5	0.96D	190B	0.042E	72.9I	9.5	17.6
	1.1 - 1.5	0.96D	190B	0.042E	72.9I	9.5	17.6
	1.1 - 1.5	0.96D	190B	0.042E	72.9I	9.5	17.6
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_20_100	20 to 100u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10100_200	100 to 200u particle size analysis, (method not recorded)
	P10200_600	200 to 600u particle size analysis, (method not recorded)
	P106002000	600 to 2000u particle size analysis, (method not recorded)
	P3A_NR	Bulk density - Not recorded