Project Name:	Geraldton land resources survey
	Project Code:	GTN	Site ID:	1424	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	04/09/89	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6850602 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	282802  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	10 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Chromosol     	Principal Profile Form:	Dr2.52
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 
	Vegetation:
	Surface Coarse 
	Profile 
	A11	0 - 0.05 m	Reddish brown (5YR4/4-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Field pH 6 (pH meter); Abrupt change to - 
	A12	0.05 - 0.1 m	Yellowish red (5YR4/6-Moist); ; Clayey sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Field pH 5.7 (pH meter); Clear change to - 
	B21	0.1 - 0.2 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 5.7 (pH 
	meter); 
	B22	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Field pH 5.7 
	(pH meter); 
	B23	0.3 - 0.4 m	Red (2.5YR4/6-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; Field pH 6.2 (pH 
	meter); 
	B24	0.4 - 0.5 m	Red (2.5YR4/6-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; Field pH 7 (pH 
	meter); 
	B25	0.5 - 0.7 m	Red (2.5YR4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Field pH 7.5 (pH meter); 
	B3	0.7 - 0.88 m	Red (2.5YR4/6-Moist); ; Sandy clay loam; Field pH 6.2 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Red duplex, some grit throughout profile layers 3-8 have many angular pores as well 0-10cm 5% ang qz 2-6mm, <2% ang qz 6-20mm 10-
	75cm <2% ang qz 6-20mm, 10% ang qz 2-6mm some Fe nodules present 75-85cm LAYER 1-4 MK, LAYER 7 LC SANDY

	Project Name:	Geraldton land resources survey
	Project Code:	GTN	Site ID:	1424	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	4.9B	7B	1.2H	0.37	0.57	0.13	0.07J	2.27D
	5.9H
	0.05 - 0.1	4.5B	4B	1.08H	0.33	0.37	0.07	0.17J	1.85D
	5.5H
	0.1 - 0.2	4.4B	5B	2.03H	0.76	0.4	0.1	0.22J	3.29D
	5.2H
	0.2 - 0.3	4.9B	6B	3.22H	1.47	0.39	0.14	0.04J	5.22D
	5.5H
	0.3 - 0.4	5.8B	6B	3.24H	2	0.28	0.18	<0.02J	5.7D
	6.2H
	0.4 - 0.5	6.2B	6B	3.42H	2.84	0.19	0.23	0.02J	6.68D
	6.8H
	0.5 - 0.7	6.4B	5B	2.73A	2.86	0.1	0.22	5.91D
	7.1H
	0.7 - 8.8	6.1B	5B	2.87H	3.52	0.14	0.31	<0.02J	6.84D
	7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	0.54D	6.2	4.3
	0.05 - 0.1	0.31D	6.6	7.7
	0.1 - 0.2	0.22D	5.8	24.4
	0.2 - 0.3	0.22D	5.6	39.6
	0.3 - 0.4	0.15D	6.3	40.5
	0.4 - 0.5	0.13D	8.2	39.4
	0.5 - 0.7	0.08D	9.7	24.6
	0.7 - 8.8	0.1D	8.3	11.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Geraldton land resources survey
	Project Code:	GTN	Site ID:	1424	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)