Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0135	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	28/04/93	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6269800 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	758960  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Sand plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Water repellent; Field pH 6.7 (pH meter); 
	A21	0.1 - 0.5 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Loose consistence; Many (20 - 50 %), Ferruginous, Coarse (6 - 20 
	mm), Concretions; Field pH 6 (pH meter); 
	B21	0.5 - 1 m	Brownish yellow (10YR6/6-Moist); Mottles, 10YR71, 0-0% , 0-5mm, Prominent; Light clay; Strong grade 
	of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Field pH
	 5.8 (pH meter); Few
	C	1 -  m	Brownish yellow (10YR6/8-Moist); Mottles, 10YR72, 10-20% , 0-5mm, Prominent; Mottles, 10YR56, 10-
	20% , 0-5mm, Prominent; Light clay; Massive grade of structure; Sandy (grains prominent) fabric; Wet; 
	Firm consistence; Field pH 5.8 (pH meter); Few
	Morphological Notes
	Observation Notes
	Site Notes
	Yellow gravel - len hill, perched water table at 180cm. Gravelly layer in a21.   

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	0135	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9B	10B	2.29H	0.44	0.08	0.07	0.03J	2.88D
	5.6H
	0.1 - 0.5	4.9B	2B	0.38H	0.21	0.02	0.04	0.05J	0.65D
	6H
	0.5 - 1	5.4B	5B	0.63H	2.1	0.1	0.23	0.02J	3.06D
	5.9H
	1 - 1	4.6B	8B	0.25H	2.46	0.05	0.3	0.14J	3.06D
	5.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.19D	69B	0.067E	1.3	3.5
	0.1 - 0.5	0.3D	19B	0.018E	0.6	4.3
	0.5 - 1	0.09D	22B	0.008E	4.6	45
	1 - 1	0.1D	21B	0.006E	8.8	53.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)