Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1156	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Tim Overheu	Locality:
	Date Desc.:	22/11/94	Elevation:	No Data
	Map Ref.:	Rainfall:	420
	Northing/Long.:	6234203 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	665737  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Limited clearing, for example selective logging
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, subangular, Granulite; 10-20%, , subrounded, Granite
	Profile 
	Ap	0 - 0.12 m	Dark yellowish brown (10YR3/4-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; 2-10%, medium gravelly, 6-20mm, subangular, Igneous rock 
	(unidentified), coarse fragments; Field pH 6.5 (pH meter); Clear change to - 
	A31	0.12 - 0.25 m	Brown (7.5YR4/4-Moist); , 0-0% ; Sandy clay loam; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; 2-10%, medium gravelly, 6-20mm, subrounded, Igneous rock (unidentified), 
	coarse fragments; Field pH 7.2 (pH meter); Gradual change to - 
	A32	0.25 - 0.5 m	Strong brown (7.5YR4/5-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; 2-10%, medium gravelly, 6-20mm, subrounded, Igneous rock (unidentified), 
	coarse fragments; Field pH 7.8 (pH meter); Abrupt change to - 
	B21	0.5 - 0.75 m	Dark red (2.5YR3/6-Moist); Mottles, 2.5YR48, 10-20% , 5-15mm, Prominent; Light medium clay; Strong 
	grade of structure, 10-20 mm, Subangular blocky; Rough-ped fabric; Moderately moist; 2-10%, medium 
	gravelly, 6-20mm, subrounded, Igneous rock (unidentified), coarse fragments; Field pH 7.8 (pH meter); 
	Clear change to - 
	D	0.75 - 1.07 m	Red (2.5YR5/6-Moist); ; Light medium clay; Moderately moist; Field pH 8.6 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Midslope of a drainage depression. Gritty yate loam. This area drains into the gairdner r. Eion mcrae   

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1156	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	5.2B	15B	5.6H	1.9	0.49	0.24	0.04J	8.23D
	5.8H
	0.12 - 0.25	5.5B	6B	1.7H	0.82	0.28	0.2	0.02J	3D
	6.4H
	0.25 - 0.5	5.8B	4B	0.94A	0.66	0.16	0.32	2.08D
	6.7H
	0.5 - 0.75	5.8B	30B	3.5A	7.8	0.32	2.8	14.42D
	6.8H
	0.75 - 1.1	7.2B	40B	3.3E	7.5	0.37	5	17B	16.17D	29.41
	8.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12	2.46D	250B	0.195E	2.3A	5.4	4.2
	0.12 - 0.25	0.3D	71B	0.028E	2.4A	4.6	3.5
	0.25 - 0.5	0.13D	48B	0.015E	2.3A	5.1	3.3
	0.5 - 0.75	0.21D	31B	0.024E	1.3A	7	29.8
	0.75 - 1.1	<2C	0.13D	54B	0.01E	1.7A	6.7	15.5
	Laboratory Analyses Completed for this profile
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Jerramungup soils inventory (=JER LRS)
	Project Code:	JSI	Site ID:	1156	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	17A1	Total Potassium - X-ray fluorescence
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)