Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0041	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	11/10/91	Elevation:	305 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6257350 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	574980  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	15 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.11
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Cultivation. Rainfed
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.08 m	Very dark brown (10YR2/2-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Dry; Field pH 6 
	(Raupach); Abundant, medium (2-5mm) roots; Abrupt, Irregular change to - 
	B21t	0.08 - 0.3 m	Pale brown (10YR6/3-Moist); Mottles, 2.5YR68, 20-50% , 5-15mm, Distinct; Fine sandy medium clay; 
	Strong grade of structure; Rough-ped fabric; Dry; Field pH 7 (Raupach); Common, fine (1-2mm) roots; 
	Clear change to - 
	B22	0.3 - 0.6 m	Yellowish red (5YR5/6-Moist); Mottles, 10YR52, 20-50% , 5-15mm, Distinct; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Dry; Field pH 5.5 (Raupach); Few, fine (1-2mm) roots; 
	Gradual change to - 
	B23	0.6 - 0.85 m	Red (2.5YR4/6-Moist); Mottles, 10YR41, 10-20% , 5-15mm, Distinct; Fine sandy medium clay; Moderate 
	grade of structure; Rough-ped fabric; Moderately moist; Field pH 5 (Raupach); Common, coarse 
	(>5mm) roots; Clear change to - 
	B3	0.85 - 0.95 m	Red (2.5YR4/6-Moist); Mottles, 5YR74, 10-20% , 5-15mm, Distinct; Light medium clay; Moderate grade 
	of structure; Rough-ped fabric; Moderately moist; 20-50%, Granite, coarse fragments; Field pH 5 
	(Raupach); Clear change to - 
	C	0.95 - 1 m	Red (2.5YR4/6-Moist); , 0-0% ; Medium clay; Moderate grade of structure; Rough-ped fabric; 
	Moderately moist; 20-50%, Granite, coarse fragments; Field pH 5 (Raupach); Clear change to - 
	Morphological Notes
	B3	FINE WEATHERED ROCK  +KS         
	C	+KS F,M ROCK FRAGMENTS         
	Observation Notes
	Site Notes
	Dolerite dyke on other side of road.  Rock at 100cm.    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0041	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.08 - 0.3	6.8B	67B	4.42A	8.71	0.41	8.71	22.25D
	7.5H
	0.08 - 0.3	6.8B	67B	4.42A	8.71	0.41	8.71	22.25D
	7.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.08 - 0.3	60I	7	33
	0.08 - 0.3	60I	7	33
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded