Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0051	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	16/10/91	Elevation:	300 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6261890 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	579200  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	315 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Hypernatric Yellow Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.02 m	Grey (10YR5/1-Moist); , 0-0% ; Loamy coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; 2-10%, Quartz, coarse fragments; Field pH 5.5 (Raupach); Abundant, medium (2-
	5mm) roots; Abrupt change to - 
	A2e	0.02 - 0.1 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; 
	Sandy (grains prominent) fabric; Dry; 20-50%, Quartz, coarse fragments; Field pH 6 (Raupach); Many, 
	medium (2-5mm) roots; Abrupt change to - 
	B21	0.1 - 0.25 m	Light yellowish brown (10YR6/4-Moist); Mottles, 5YR58, 10-20% , 0-5mm, Faint; Sandy medium clay; 
	Strong grade of structure; Rough-ped fabric; Dry; Field pH 7 (Raupach); Common, fine (1-2mm) roots; 
	Clear change to - 
	B22	0.25 - 0.45 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5YR48, 0-2% , 0-5mm, Distinct; Sandy medium clay; Strong
	 grade of structure; Smooth-ped fabric; Dry; Field pH 8.5 (Raupach); Common, fine (1-2mm) roots; Clear
	 change to - 
	B23t	0.45 - 0.75 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5YR48, 2-10% , 5-15mm, Distinct; Medium clay; Moderate 
	grade of structure; Smooth-ped fabric; Moderately moist; Field pH 8.5 (Raupach); Gradual change to - 
	B3	0.75 - 0.9 m	Yellow (10YR8/6-Moist); Mottles, 7.5R36, 10-20% , 5-15mm, Prominent; Medium clay; Moderate grade 
	of structure; Smooth-ped fabric; Moderately moist; Field pH 8.5 (Raupach); Gradual change to - 
	C	0.9 - 1.1 m	White (10YR8/2-Moist); Mottles, 10YR86, 20-50% , 5-15mm, Distinct; Medium clay; Moderate grade of 
	structure; Smooth-ped fabric; Moderately moist; Field pH 8 (Raupach); 
	Morphological Notes
	A1	GRAVEL F,A         
	A2e	GRAVEL FA & FEW M,C R,IS         
	B21	SAMPLED         
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0051	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.1 - 0.25	6.7B	17B	1.88A	3.7	0.24	1.96	7.78D
	8H
	0.1 - 0.25	6.7B	17B	1.88A	3.7	0.24	1.96	7.78D
	8H
	0.1 - 0.25	6.7B	17B	1.88A	3.7	0.24	1.96	7.78D
	8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.1 - 0.25	<2C	57I	3	40
	0.1 - 0.25	<2C	57I	3	40
	0.1 - 0.25	<2C	57I	3	40
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded