Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0057	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	18/10/91	Elevation:	325 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6254030 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	566090  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	35 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	270 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.32
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Cultivation. Rainfed
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Loamy sand; Weak grade of structure; Rough-ped fabric; 
	Dry; 2-10%, Quartz, coarse fragments; Water repellent; Field pH 6 (Raupach); Many, fine (1-2mm) 
	roots; Clear change to - 
	A2j	0.1 - 0.15 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Clayey coarse sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Dry; Field pH 7 (Raupach); Few, fine (1-2mm) roots; Abrupt change to - 
	B21t	0.15 - 0.5 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5YR48, 10-20% , 5-15mm, Distinct; Medium clay; Strong 
	grade of structure, Polyhedral; Smooth-ped fabric; Dry; Field pH 7 (Raupach); Common, fine (1-2mm) 
	roots; Clear change to - 
	B22t	0.5 - 0.6 m	Yellowish brown (10YR5/4-Moist); Mottles, 2.5YR48, 10-20% , 0-5mm, Distinct; Medium clay; Strong 
	grade of structure, Polyhedral; Smooth-ped fabric; Dry; Field pH 7.5 (Raupach); Common, coarse 
	(>5mm) roots; 
	Morphological Notes
	A1	F A QZ +KS         
	A2j	SPORADIC BLEACH 10YR7/2d         
	B21t	SAMPLED +S         
	Observation Notes
	Site Notes
	Hole dug on road reserve next to lupin crop - not performing well    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0057	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.15 - 0.5	6.3B	12B	0.75A	2.68	0.2	0.94	4.57D
	7.4H
	0.15 - 0.5	6.3B	12B	0.75A	2.68	0.2	0.94	4.57D
	7.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.15 - 0.5	44I	4	52
	0.15 - 0.5	44I	4	52
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded