Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0058	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	18/10/91	Elevation:	310 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6256600 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	566240  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	20 metres
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.12 m	Very dark brown (10YR2/2-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; 20-50%, Ironstone, coarse fragments; Common (10 - 20 %), Ferruginous, 
	Coarse (6 - 20 mm), Nodules; Common (10 - 20 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; 
	Common (10 - 20 %), Ferruginous, Extremely coarse (> 60 mm), Nodules; Water repellent; Field pH 6 
	(Raupach); Abundant, fine (1-2mm) roots; 
	A21e	0.12 - 0.5 m	Pale brown (10YR6/3-Moist); , 0-0% ; Single grain grade of structure; Sandy (grains prominent) fabric; 
	Dry; 50-90%, Ironstone, coarse fragments; Very many (50 - 100 %), Ferruginous, Coarse (6 - 20 mm), 
	Nodules; Very many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Very many (50 - 100 
	%), Ferruginous, Extremely coarse (> 60 mm), Nodules; Water repellent; Field pH 6 (Raupach); Many, 
	fine (1-2mm) roots; Gradual change to - 
	A22e	0.5 - 0.65 m	Pale brown (10YR6/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; 50-90%, Ironstone, coarse fragments; Many (20 - 50 %), 
	Ferruginous, Medium (2 -6 mm), Nodules; Many (20 - 50 %), Ferruginous, Fine (0 - 2 mm), Nodules; 
	Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7 (Raupach); Common, fine (1-
	2mm) roots; Clear change to - 
	B21	0.65 - 0.9 m	Pale brown (10YR6/3-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Distinct; Sandy light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; 20-50%, Ironstone, coarse fragments;
	 Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Many (20 - 50 %), Ferruginous, Very 
	coarse (20 - 60 mm), Nodules; Field pH 7.5 (Raupach); Few, fine (1-2mm) roots; Gradual change to - 
	B22	0.9 - 1.05 m	Light grey (10YR7/1-Moist); Mottles, 10YR68, 10-20% , 5-15mm, Distinct; Medium clay; Moderate 
	grade of structure; Rough-ped fabric; Moderately moist; 20-50%, Ironstone, coarse fragments; Common 
	(10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7 (Raupach); 
	Morphological Notes
	A1	F,M,C IS         
	A21e	F,M,C A QZ IS R +CS         
	A22e	F,M IR  R,S         
	B21	M IS  SAMPLED         
	B22	M IS         
	Observation Notes
	Site Notes
	Surface water repellence due to clovers    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0058	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.65 - 0.9	6.1B	11B	0.8A	3.7	0.07	0.94	5.51D
	7.2H
	0.65 - 0.9	6.1B	11B	0.8A	3.7	0.07	0.94	5.51D
	7.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.65 - 0.9	65I	5.5	29.5
	0.65 - 0.9	65I	5.5	29.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded