Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0066	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	24/10/91	Elevation:	311 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6257250 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	582060  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	10 metres
	Elem. Type:	Summit surface	Slope Category:	No Data
	Slope:	1 % 	Aspect:	225 degrees
	Surface Soil Condition 	Soft
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Magnesic-Natric Grey Kurosol     	Principal Profile Form:	Dg2.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A	0 - 0.11 m	Greyish brown (10YR5/2-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Dry; Water 
	repellent; Field pH 6 (Raupach); Abundant, very fine (0-1mm) roots; Sharp, Wavy change to - 
	2A1	0.11 - 0.16 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; 2-10%, Quartz, coarse fragments; Water repellent; Field pH 5.5 (Raupach); 
	Abundant, very fine (0-1mm) roots; Sharp, Wavy change to - 
	2A2e	0.16 - 0.4 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Clayey coarse sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Dry; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Clear change to - 
	2B21	0.4 - 0.83 m	White (10YR8/1-Moist); Mottles, 10R46, 20-50% , 5-15mm, Distinct; Medium clay; Moderate grade of 
	structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Field pH 6 (Raupach); Common, medium (2-
	5mm) roots; Clear change to - 
	2B22	0.83 - 1.48 m	Light grey (10YR7/1-Moist); , 0-0% ; Light medium clay; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Smooth-ped fabric; Dry; 20-50%, Quartz, coarse fragments; Field pH 6 (Raupach); Few, 
	medium (2-5mm) roots; Clear, Tongued change to - 
	C	1.48 - 1.8 m	White (10YR8/1-Moist); , 0-0% ; Light medium clay; Massive grade of structure; Rough-ped fabric; Dry; 
	10-20%, Quartz, coarse fragments; Field pH 6 (Raupach); 
	Morphological Notes
	A	DEPOSITED WIND BLOWN SAND
	2A1	F A QZ
	2B21	+S
	2B22	F A QZ
	C	F A QZ +S
	Observation Notes
	Site Notes
	Site in remnant veg. On laneway.  Hardsetting on near pasture

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0066	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.4B	4B
	5.3H
	0 - 0.1	4.4B	4B
	5.3H
	0.11 - 0.16	4.8B	4B	1.61H	0.52	0.09	0.09	0.09J	2.31D
	6H
	0.11 - 0.16	4.8B	4B	1.61H	0.52	0.09	0.09	0.09J	2.31D
	6H
	0.16 - 0.4	4.6B	4B	0.32H	0.23	0.03	0.09	0.07J	0.67D
	5.7H
	0.16 - 0.4	4.6B	4B	0.32H	0.23	0.03	0.09	0.07J	0.67D
	5.7H
	0.4 - 0.83	5.3B	73B	0.36H	4.51	0.07	1.59	0.08J	6.53D
	5.5H
	0.4 - 0.6	5.1B	160B	0.47H	4.79	0.08	1	0.05J	6.34D
	5.4H
	0.4 - 0.83	5.3B	73B	0.36H	4.51	0.07	1.59	0.08J	6.53D
	5.5H
	0.4 - 0.6	5.1B	160B	0.47H	4.79	0.08	1	0.05J	6.34D
	5.4H
	0.6 - 0.83	5.2B	140B	0.25H	4.45	0.03	1.36	0.03J	6.09D
	5.4H
	0.6 - 0.83	5.2B	140B	0.25H	4.45	0.03	1.36	0.03J	6.09D
	5.4H
	0.83 - 1.48	5.6B	130B	0.11H	6.52	0.02	3.65	0.04J	10.3D
	6H
	0.83 - 1.48	5.6B	130B	0.11H	6.52	0.02	3.65	0.04J	10.3D
	6H
	1.48 - 1.8	5.5B	140B	0.07H	5.22	<0.02	2.72	0.03J	8.02D
	5.9H
	1.48 - 1.8	5.5B	140B	0.07H	5.22	<0.02	2.72	0.03J	8.02D
	5.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.07D	110B	0.064E
	0 - 0.1	1.07D	110B	0.064E
	0.11 - 0.16	1.15D	76B	1.6	4.1
	0.11 - 0.16	1.15D	76B	1.6	4.1
	0.16 - 0.4	0.3D	29B	3.7	3.1
	0.16 - 0.4	0.3D	29B	3.7	3.1
	0.4 - 0.83	0.16D	32B	2.8	62
	0.4 - 0.6	41I	2.5	56.5
	0.4 - 0.83	0.16D	32B	2.8	62
	0.4 - 0.6	41I	2.5	56.5
	0.6 - 0.83	46I	4	50
	0.6 - 0.83	46I	4	50
	0.83 - 1.48	0.06D	31B	11.9	64
	0.83 - 1.48	0.06D	31B	11.9	64

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0066	Observation 	1
	Agency Name:	Agriculture Western Australia
	1.48 - 1.8	0.05D	40B	26.2	42.6
	1.48 - 1.8	0.05D	40B	26.2	42.6
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)