Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0071	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	25/10/91	Elevation:	309 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6260890 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	587520  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	225 degrees
	Surface Soil Condition 	Soft
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy4.81
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A11	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Clayey fine sand; Single grain grade of structure; 
	Dry; 0-2%, Ironstone, coarse fragments; Water repellent; Field pH 6 (Raupach); Abundant, fine (1-2mm) 
	roots; Clear change to - 
	A12	0.12 - 0.25 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Clayey fine sand; Single grain grade of structure; Dry; 50-
	90%, Ironstone, coarse fragments; Very many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), 
	Nodules; Water repellent; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Clear change to - 
	A2ec	0.25 - 0.43 m	Pale brown (10YR6/3-Moist); , 0-0% ; Single grain grade of structure; Dry; 50-90%, Ironstone, coarse 
	fragments; Very many (50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Abrupt change to - 
	B2tc	0.43 - 0.55 m	Reddish yellow (7.5YR6/6-Moist); , 0-0% ; Massive grade of structure; Rough-ped fabric; Dry; 50-90%, 
	Ironstone, coarse fragments; Very many (50 - 100 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field 
	pH 6 (Raupach); Few, medium (2-5mm) roots; 
	Morphological Notes
	A11	M R GC         
	A12	M,C U GC         
	A2ec	M,C U GC   +KS         
	B2tc	M U IS  SAMPLED +SLC         
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0071	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.43 - 0.55	5.7B	7B	1.66H	2.31	0.19	0.56	<0.02J	4.72D
	6.9H
	0.43 - 0.55	5.7B	7B	1.66H	2.31	0.19	0.56	<0.02J	4.72D
	6.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.43 - 0.55	76.5I	3.5	20
	0.43 - 0.55	76.5I	3.5	20
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded