Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0108	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	14/11/91	Elevation:	321 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6261250 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	556620  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	30 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition 	Soft
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.07 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; 
	Moderately moist; 2-10%, Quartz, coarse fragments; Water repellent; Field pH 6 (Raupach); Many, fine 
	(1-2mm) roots; Abrupt change to - 
	A2	0.07 - 0.16 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Clayey sand; Dry; 10-20%, Quartz, coarse fragments; 
	Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Abrupt change to - 
	B21	0.16 - 0.5 m	Yellowish brown (10YR5/6-Moist); , 2.5Y54, 10-20% , 0-5mm, Faint; Medium heavy clay; Strong grade of 
	structure, 20-50 mm, Polyhedral; Smooth-ped fabric; Dry; Field pH 5 (Raupach); Many, fine (1-2mm) 
	roots; Clear change to - 
	B22	0.5 - 0.6 m	Strong brown (7.5YR5/6-Moist); Mottles, 7.5YR78, 10-20% , 5-15mm, Distinct; Medium heavy clay; 
	Moderate grade of structure, 20-50 mm, Polyhedral; Smooth-ped fabric; Dry; Field pH 5 (Raupach); 
	Common, fine (1-2mm) roots; Gradual change to - 
	B23	0.6 - 0.85 m	Strong brown (7.5YR4/6-Moist); Mottles, 10YR42, 10-20% , 5-15mm, Faint; Sandy light medium clay; 
	Weak grade of structure; Rough-ped fabric; Dry; Field pH 5.5 (Raupach); Gradual change to - 
	B3	0.85 - 1 m	Yellowish red (5YR5/6-Moist); Mottles, 10YR53, 10-20% , 5-15mm, Faint; Medium clay; Weak grade of 
	structure; Rough-ped fabric; Dry; Field pH 5 (Raupach); 
	Morphological Notes
	A1	F A QZ R GC
	A2	F A QZ &M R GC
	B21	SAMPLED
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0108	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.16 - 0.5	4.9B	5B	0.35H	2.98	0.04	0.53	0.04J	3.9D
	6.1H
	0.16 - 0.5	4.9B	5B	0.35H	2.98	0.04	0.53	0.04J	3.9D
	6.1H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.16 - 0.5	59I	5.5	35.5
	0.16 - 0.5	59I	5.5	35.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded