Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0133	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	28/11/91	Elevation:	275 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6273920 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	567940  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	2 metres
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Hypernatric Grey Sodosol     	Principal Profile Form:	Dy2.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Dry; 
	Field pH 6.5 (Raupach); Abundant, very fine (0-1mm) roots; Abrupt change to - 
	A2e	0.08 - 0.28 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moderately moist; 
	0-2%, Quartz, coarse fragments; Field pH 7 (Raupach); Many, fine (1-2mm) roots; Abrupt change to - 
	B2	0.28 - 0.55 m	Pale brown (10YR6/3-Moist); Mottles, 2.5YR46, 2-10% , 5-15mm, Prominent; Sandy medium clay; Strong
	 grade of structure, 200-500 mm, Columnar; Rough-ped fabric; Dry; Field pH 8.5 (Raupach); Gradual 
	change to - 
	C11	0.55 - 0.8 m	Pale brown (10YR6/3-Moist); Mottles, 2.5YR46, 10-20% , 5-15mm, Prominent; Sandy clay loam; Rough-
	ped fabric; Moderately moist; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Soft segregations; 
	Field pH 8.5 (Raupach); Clear change to - 
	C12	0.8 - 1.05 m	Very pale brown (10YR7/4-Moist); Mottles, 5YR58, 2-10% , 5-15mm, Distinct; Sandy light clay; Rough-
	ped fabric; Moderately moist; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; Field 
	pH 8 (Raupach); Clear change to - 
	C13	1.05 - 1.1 m	Very pale brown (10YR7/3-Moist); Mottles, 5YR58, 20-50% , 5-15mm, Distinct; , N50; Clay loam, fine 
	sandy; Rough-ped fabric; Moist; Field pH 8 (Raupach); 
	Morphological Notes
	A1	F S QZ (<0.5%) GRAVEL         
	A2e	F S QZ         
	B2	SAMPLED         
	Observation Notes
	Site Notes
	Site on roadside-landuse to east is grazing, to west is cropping(oats)    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0133	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.28 - 0.55	7.1B	65B	1.98E	4.34	0.08	2.51	10B	8.91D	25.10
	8.1H
	0.28 - 0.55	7.1B	65B	1.98E	4.34	0.08	2.51	10B	8.91D	25.10
	8.1H
	0.28 - 0.55	7.1B	65B	1.98E	4.34	0.08	2.51	10B	8.91D	25.10
	8.1H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.28 - 0.55	<2C	63I	3.5	33.5
	0.28 - 0.55	<2C	63I	3.5	33.5
	0.28 - 0.55	<2C	63I	3.5	33.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded