Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0150	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	26/03/92	Elevation:	295 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6252810 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	487480  Datum: AGD84	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	25 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	6 % 	Aspect:	135 degrees
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Ferric Bleached-Orthic Tenosol     	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.15 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Water repellent; Field pH 5 (Raupach); Common, fine (1-2mm) roots; Abrupt, Wavy change to
	 - 
	A2e	0.15 - 0.5 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Field pH 7 (Raupach); Few, coarse (>5mm) roots; Gradual, Tongued change to - 
	B1	0.5 - 0.9 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Few (2 - 10 %), Ferruginous, Extremely coarse (> 60 mm), Nodules; Field pH 6.5
	 (Raupach); Many, medium (2-5mm) roots; Clear, Smooth change to - 
	B2c	0.9 - 1.2 m	Yellow (10YR7/6-Moist); Mottles, 10YR68, 10-20% , 15-30mm, Distinct; Coarse sand; Single grain 
	grade of structure; Sandy (grains prominent) fabric; Dry; 50-90%, subrounded, Ironstone, coarse 
	fragments; Very many (50 - 100 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Field pH 7 
	(Raupach); Few, fine (1-2mm) roots; Clear, Irregular change to - 
	B3	1.2 - 1.5 m	Yellow (2.5Y7/6-Moist); Mottles, 7.5YR58, 10-20% , 15-30mm, Distinct; Sandy clay loam; Massive grade 
	of structure; Moderately moist; 20-50%, subrounded, Ironstone, coarse fragments; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7.5 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	B1	+ COARSE SAND
	B3	MOIST BELOW 150CM. SUBPLASTIC
	Observation Notes
	Site Notes
	[ignored B3 (SCL layer) in classification, otherwise Basic Ferric Yellow Chromosol]

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0150	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.6B	3B	1.13H	0.16	0.03	0.03	0.14J	1.35D
	5.7H
	0 - 0.1	4.7B	3B
	5.9H
	0 - 0.15	4.6B	3B	1.13H	0.16	0.03	0.03	0.14J	1.35D
	5.7H
	0 - 0.1	4.7B	3B
	5.9H
	0.15 - 0.5	5B	1B	0.13H	0.08	<0.02	<0.02	0.04J	0.23D
	6.1H
	0.15 - 0.5	5B	1B	0.13H	0.08	<0.02	<0.02	0.04J	0.23D
	6.1H
	0.5 - 0.9	5.2B	2B	0.26H	0.27	0.02	0.06	0.06J	0.61D
	6.4H
	0.5 - 0.9	5.2B	2B	0.26H	0.27	0.02	0.06	0.06J	0.61D
	6.4H
	0.9 - 1.2	5.6B	3B	0.35H	0.58	0.13	0.22	0.02J	1.28D
	6.6H	2B	0.23A	0.68	0.11	0.24	1.26D
	5.7B
	6.8H
	0.9 - 1.2	5.6B	3B	0.35H	0.58	0.13	0.22	0.02J	1.28D
	6.6H	2B	0.23A	0.68	0.11	0.24	1.26D
	5.7B
	6.8H
	0.9 - 1.2	5.6B	3B	0.35H	0.58	0.13	0.22	0.02J	1.28D
	6.6H	2B	0.23A	0.68	0.11	0.24	1.26D
	5.7B
	6.8H
	0.9 - 1.2	5.6B	3B	0.35H	0.58	0.13	0.22	0.02J	1.28D
	6.6H	2B	0.23A	0.68	0.11	0.24	1.26D
	5.7B
	6.8H
	1.2 - 1.5	6.1B	3B	0.04A	1.9	<0.02	0.24	2.19D
	6.7H
	1.2 - 1.5	6.1B	3B	0.04A	1.9	<0.02	0.24	2.19D
	6.7H
	1.2 - 1.5	6.1B	3B	0.04A	1.9	<0.02	0.24	2.19D
	6.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	0.5D	52B	0.028E	0.3	1.6
	0 - 0.1	1.06D	79B	0.061E
	0 - 0.15	0.5D	52B	0.028E	0.3	1.6
	0 - 0.1	1.06D	79B	0.061E
	0.15 - 0.5	0.09D	19B	0.006E	0.7	0.9
	0.15 - 0.5	0.09D	19B	0.006E	0.7	0.9
	0.5 - 0.9	0.14D	18B	0.01E	0.4	6.1
	0.5 - 0.9	0.14D	18B	0.01E	0.4	6.1

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0150	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.9 - 1.2	0.16D	35B	0.011E	1.3	6.1
	0.2D	41B	0.012E	1.9	6.1
	0.9 - 1.2	0.16D	35B	0.011E	1.3	6.1
	0.2D	41B	0.012E	1.9	6.1
	0.9 - 1.2	0.16D	35B	0.011E	1.3	6.1
	0.2D	41B	0.012E	1.9	6.1
	0.9 - 1.2	0.16D	35B	0.011E	1.3	6.1
	0.2D	41B	0.012E	1.9	6.1
	1.2 - 1.5	0.16D	30B	0.01E	1.7	22
	1.2 - 1.5	0.16D	30B	0.01E	1.7	22
	1.2 - 1.5	0.16D	30B	0.01E	1.7	22
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)