Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0242	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	02/06/92	Elevation:	250 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6283430 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	507790  Datum: AGD84	Drainage:	Rapidly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Alluvial plain
	Morph. Type:	Lower-slope	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.23
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A11	0 - 0.12 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 5 (Raupach); Many, very fine (0-1mm) roots; Sharp, Smooth change to - 
	A12	0.12 - 0.25 m	Light grey (10YR7/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Loose consistence; 
	Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Abrupt change to - 
	A21e	0.25 - 1 m	Pale yellow (2.5Y7/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Loose consistence; 
	Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Abrupt change to - 
	A22ec	1 - 1.1 m	Pale yellow (2.5Y7/4-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Moist; Loose 
	consistence; 50-90%, coarse gravelly, 20-60mm, subangular, , coarse fragments; Many (20 - 50 %), 
	Ferruginous, Extremely coarse (> 60 mm), Nodules; Field pH 6 (Raupach); Common, very fine (0-1mm) 
	roots; Abrupt change to - 
	A3e	1.1 - 1.15 m	Pale yellow (2.5Y7/4-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; Loose 
	consistence; 2-10%, fine gravelly, 2-6mm, subrounded, , coarse fragments; Few (2 - 10 %), Ferruginous,
	 Fine (0 - 2 mm), Nodules; Field pH 6 (Raupach); Clear change to - 
	B2t	1.15 - 1.3 m	Pale yellow (2.5Y7/4-Moist); Mottles, 10YR68, 10-20% , 5-15mm, Faint; Clayey sand; Single grain grade
	 of structure; Moist; Loose consistence; Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), Nodules;
	 Field pH 6 (Raupach); 
	Morphological Notes
	B2t	Sampled for % clay         
	Observation Notes
	Site Notes

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0242	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.56B
	0.16 - 0.26	4.64B
	0.41 - 0.51	4.82B
	1.15 - 1.3	5.9B	9B
	6.7H
	1.15 - 1.3	5.9B	9B
	6.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.41 - 0.51
	1.15 - 1.3
	1.15 - 1.3
	Laboratory Analyses Completed for this profile
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)