Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0318	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	15/07/92	Elevation:	320 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6273000 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	543310  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	180 degrees
	Surface Soil Condition 	Firm
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Moderately moist;
	 Loose consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Field pH 6 
	(Raupach); Abundant, very fine (0-1mm) roots; Sharp, Smooth change to - 
	A21	0.1 - 0.3 m	Brownish yellow (10YR6/6-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; 
	Moderately moist; Loose consistence; Field pH 5.5 (Raupach); Many, very fine (0-1mm) roots; Abrupt 
	change to - 
	A22e	0.3 - 0.5 m	Pale yellow (2.5Y7/3-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; Wet; Loose 
	consistence; Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Abrupt, Wavy change to - 
	B21	0.5 - 0.65 m	Yellow (10YR7/6-Moist); Mottles, 10R46, 20-50% , 0-5mm, Distinct; Coarse sandy light clay; Moderate 
	grade of structure; Rough-ped fabric; Moist; Weak consistence; Field pH 6.5 (Raupach); Common, very 
	fine (0-1mm) roots; Clear change to - 
	B22	0.65 - 1 m	Reddish yellow (7.5YR6/8-Moist); Mottles, 10R48, 10-20% , 0-5mm, Distinct; Medium clay; Moderate 
	grade of structure; Rough-ped fabric; Moist; Firm consistence; Soil matrix is Slightly calcareous; Field 
	pH 7 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	A22e	Water entered about clay         
	B21	Sampled for ESP         
	B22	Sporadic white (kaolinite) patches from 80cm         
	Observation Notes
	Site Notes
	Along House Road EC=28ms/m    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0318	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.41B
	0.16 - 0.26	4.05B
	0.41 - 0.51	4.38B
	0.5 - 0.65	4.7B	4B	0.48H	0.88	0.04	0.14	0.09J	1.54D
	5.7H
	0.5 - 0.65	4.7B	4B	0.48H	0.88	0.04	0.14	0.09J	1.54D
	5.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.41 - 0.51
	0.5 - 0.65	69I	3.5	27.5
	0.5 - 0.65	69I	3.5	27.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded