Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0321	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	15/07/92	Elevation:	360 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6275860 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	546310  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	40 metres
	Elem. Type:	Summit surface	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.11
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.12 m	Dark brown (10YR3/3-Moist); , 0-0% ; Sandy clay loam; Single grain grade of structure; Moderately 
	moist; Loose consistence; Field pH 6 (Raupach); Abundant, fine (1-2mm) roots; Sharp, Wavy change to - 
	B21t	0.12 - 0.3 m	Red (2.5YR5/8-Moist); Mechanical, 10YR32, 10-20% , 0-5mm, Faint; Substrate influence, 10YR81, 2-
	10% , 0-5mm, Distinct; Medium clay; Strong grade of structure; Smooth-ped fabric; Dry; Field pH 7.5 
	(Raupach); Common, very fine (0-1mm) roots; Diffuse change to - 
	B22t	0.3 - 0.7 m	Red (2.5YR5/8-Moist); Substrate influence, 10YR81, 10-20% , 0-5mm, Distinct; Medium clay; Moderate 
	grade of structure; Rough-ped fabric; Dry; Field pH 7 (Raupach); Common, very fine (0-1mm) roots; 
	Clear change to - 
	C	0.7 -  m	White (10YR8/1-Moist); Mottles, 5YR58, 10-20% , 0-5mm, Distinct; Clay loam; Massive grade of 
	structure; Dry; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	A1	5 clay         
	B21t	% clay ESP         
	B22t	Kaolinitic
	C	Kaolinitic
	Observation Notes
	Site Notes
	Tuck Rd    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0321	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	5.8B	12B
	6.6H
	0 - 0.12	5.8B	12B
	6.6H
	0 - 0.11	5.49B
	0.12 - 0.3	6.4B	23B	3.53A	5.61	0.12	0.82	10.08D
	7.1H
	0.12 - 0.3	6.4B	23B	3.53A	5.61	0.12	0.82	10.08D
	7.1H
	0.16 - 0.26	6.51B
	0.41 - 0.51	6.29B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0 - 0.12
	0 - 0.11
	0.12 - 0.3	35.5I	7.5	57
	0.12 - 0.3	35.5I	7.5	57
	0.16 - 0.26
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded