Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0329	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	17/07/92	Elevation:	327 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6278420 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	546760  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	50 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	180 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.15 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; Clear change to - 
	A21e	0.15 - 0.25 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Moist; 
	Loose consistence; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Abrupt change to - 
	A22ec	0.25 - 0.4 m	Pale brown (10YR6/3-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Moist; Loose 
	consistence; 50-90%, medium gravelly, 6-20mm, rounded, , coarse fragments; Field pH 6 (Raupach); 
	Few, very fine (0-1mm) roots; Abrupt change to - 
	B2t	0.4 - 0.6 m	Strong brown (7.5YR5/7-Moist); Mottles, 2.5YR57, 10-20% , 5-15mm, Distinct; Coarse sandy clay loam; 
	Massive grade of structure; Dry; Very firm consistence; 20-50%, coarse gravelly, 20-60mm, subrounded, 
	, coarse fragments; Many (20 - 50 %), Ferruginous, Very coarse (20 - 60 mm), Nodules; Field pH 6 
	(Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A22ec	Includes some coarse smoothfaced gravel         
	B2t	Very slight dispersion. Sampled % clay,ESP. Too dry and hard to auger         
	Observation Notes
	Site Notes
	Trimmer Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0329	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.53B
	0.16 - 0.26	4.33B
	0.4 - 0.6	4.8B	3B	0.8H	0.85	0.05	0.21	0.17J	1.91D
	6H
	0.4 - 0.6	4.8B	3B	0.8H	0.85	0.05	0.21	0.17J	1.91D
	6H
	0.41 - 0.51	4.85B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.4 - 0.6	84.5I	4	11.5
	0.4 - 0.6	84.5I	4	11.5
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded