Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0434	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	09/09/92	Elevation:	275 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6281540 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	563600  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.12 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Abrupt change to - 
	A2e	0.12 - 0.4 m	Pale brown (10YR6/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Wet; Loose consistence; 
	20-50%, medium gravelly, 6-20mm, subrounded, , coarse fragments; Field pH 6.5 (Raupach); Common, 
	fine (1-2mm) roots; Abrupt change to - 
	B21t	0.4 - 0.6 m	Grey (10YR6/1-Moist); Mottles, 10YR68, 20-50% , 15-30mm, Distinct; Light clay; Moderate grade of 
	structure; Smooth-ped fabric; Moderately moist; Firm consistence; Field pH 6.5 (Raupach); Common, 
	fine (1-2mm) roots; Clear change to - 
	B22t	0.6 - 1.05 m	Brownish yellow (10YR6/7-Moist); Mottles, 2.5Y63, 10-20% , 0-5mm, Distinct; Light clay; Weak grade of 
	structure; Rough-ped fabric; Dry; Weak consistence; Field pH 7 (Raupach); Common, fine (1-2mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	Guidera Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0434	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	5.25B
	0.16 - 0.26	4.91B
	0.4 - 0.6	5.7B	17B	1.63A	2.88	0.33	1.51	6.35D
	6.6H
	0.4 - 0.6	5.7B	17B	1.63A	2.88	0.33	1.51	6.35D
	6.6H
	0.41 - 0.51	5.59B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.4 - 0.6
	0.4 - 0.6
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)