Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0450	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	14/09/92	Elevation:	301 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6245020 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	562890  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	25 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	315 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dg2.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.12 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 10-20%, medium gravelly, 6-20mm, rounded, , coarse fragments; Few (2 - 10 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Clear 
	change to - 
	A2e	0.12 - 0.4 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Moist; Loose 
	consistence; 50-90%, medium gravelly, 6-20mm, rounded, , coarse fragments; Very many (50 - 100 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 6.5 (Raupach); Common, fine (1-2mm) roots; 
	Abrupt change to - 
	B21t	0.4 - 0.5 m	Pale yellow (2.5Y7/4-Moist); Mottles, 10YR68, 20-50% , 15-30mm, Distinct; Light medium clay; Moderate
	 grade of structure; Rough-ped fabric; Weak consistence; 10-20%, medium gravelly, 6-20mm, rounded, , 
	coarse fragments; 2-10%, coarse gravelly, 20-60mm, subrounded, , coarse fragments; Common (10 - 20 
	%), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 8 (Raupach); Common, fine (1-2mm) roots; 
	Clear change to - 
	B22t	0.5 - 0.6 m	Pale yellow (2.5Y7/4-Moist); Mottles, 10R46, 10-20% , 30-mm, Prominent; Medium clay; Moderate grade
	 of structure; Rough-ped fabric; Moist; Weak consistence; 10-20%, medium gravelly, 6-20mm, rounded, , 
	coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 8.5 (Raupach); 
	Clear change to - 
	B3	0.6 - 0.9 m	Light grey (10YR7/1-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Distinct; Light clay; Weak grade of 
	structure; Rough-ped fabric; Moist; Weak consistence; 10-20%, medium gravelly, 6-20mm, rounded, , 
	coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 9 (Raupach); 
	Clear change to - 
	Morphological Notes
	B21t	Very slight dispersion         
	B3	Water entered at 60cm         
	Observation Notes
	Site Notes
	Peringillup East Road    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0450	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	4.87B
	0.16 - 0.26	5.68B
	0.4 - 0.6	6.6B	11B	1.39A	3.67	0.1	1.06	6.22D
	7.6H	1.39A	3.67	0.1	1.06	6.22D
	6.6B
	7.6H
	0.4 - 0.6	6.6B	11B	1.39A	3.67	0.1	1.06	6.22D
	7.6H	1.39A	3.67	0.1	1.06	6.22D
	6.6B
	7.6H
	0.41 - 0.51	6.26B
	0.4 - 0.6	6.6B	11B	1.39A	3.67	0.1	1.06	6.22D
	7.6H	1.39A	3.67	0.1	1.06	6.22D
	6.6B
	7.6H
	0.4 - 0.6	6.6B	11B	1.39A	3.67	0.1	1.06	6.22D
	7.6H	1.39A	3.67	0.1	1.06	6.22D
	6.6B
	7.6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.16 - 0.26
	0.4 - 0.6
	0.4 - 0.6
	0.41 - 0.51
	0.4 - 0.6
	0.4 - 0.6
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)