Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0489	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	22/09/92	Elevation:	253 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6239540 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	582510  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	25 metres
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	A1	0 - 0.05 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy fine sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Abrupt, Smooth change to - 
	A2e	0.05 - 0.12 m	Brown (10YR5/3-Moist); , 0-0% ; Clayey fine sand; Single grain grade of structure; Moist; Loose 
	consistence; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Wavy change to - 
	B21	0.12 - 0.2 m	Yellowish red (5YR4/6-Moist); Mottles, 10YR64, 10-20% , 5-15mm, Faint; Sandy light medium clay; 
	Strong grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 8.5 
	(Raupach); Many, fine (1-2mm) roots; Clear change to - 
	B22	0.2 - 0.5 m	Light yellowish brown (10YR6/4-Moist); Mottles, 7.5YR56, 20-50% , 5-15mm, Distinct; Sandy medium 
	clay; Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 9.5 
	(Raupach); Common, very fine (0-1mm) roots; Clear change to - 
	B23k	0.5 - 0.7 m	Light yellowish brown (10YR6/4-Moist); Mottles, 7.5YR56, 20-50% , 5-15mm, Distinct; Light clay; 
	Moderate grade of structure; Rough-ped fabric; Dry; Very firm consistence; Common (10 - 20 %), 
	Calcareous, Coarse (6 - 20 mm), Concretions; Few (2 - 10 %), Calcareous, Extremely coarse (> 60 
	mm), Concretions; Soil matrix is Highly calcareous; Field pH 9.5 (Raupach); Few, very fine (0-1mm) 
	roots; Clear change to - 
	B3k	0.7 - 0.8 m	Pale yellow (2.5Y7/3-Moist); Mottles, 7.5YR56, 10-20% , 5-15mm, Distinct; Medium clay; Moderate 
	grade of structure; Smooth-ped fabric; Dry; Strong consistence; Few (2 - 10 %), Calcareous, Extremely 
	coarse (> 60 mm), Concretions; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; 
	Soil matrix is Moderately calcareous; Field pH 9.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Pallinup Road - on roadside    	

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0489	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	6.53B
	0.13 - 0.21	6.59B
	0.12 - 0.3	7.2B	35B	1.29E	6.19	0.46	3.12	12B	11.06D	26.00
	8.4H
	0.12 - 0.3	7.2B	35B	1.29E	6.19	0.46	3.12	12B	11.06D	26.00
	8.4H
	0.12 - 0.3	7.2B	35B	1.29E	6.19	0.46	3.12	12B	11.06D	26.00
	8.4H
	0.41 - 0.51	8.06B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11
	0.13 - 0.21
	0.12 - 0.3	<2C
	0.12 - 0.3	<2C
	0.12 - 0.3	<2C
	0.41 - 0.51
	Laboratory Analyses Completed for this profile
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)