Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0902	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	16/06/93	Elevation:	335 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6286020 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	577660  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	30 metres
	Elem. Type:	Summit surface	Slope Category:	No Data
	Slope:	2 % 	Aspect:	180 degrees
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy5.62
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	10-20%, medium gravelly, 6-20mm, rounded, ; No surface coarse fragments
	Profile 
	A1p	0 - 0.12 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, rounded, , coarse fragments; 10-20%, medium gravelly, 6-
	20mm, subrounded, , coarse fragments; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Abrupt 
	change to - 
	A2	0.12 - 0.35 m	Brown (10YR5/3-Moist); , 0-0% ; Sandy loam; Single grain grade of structure; Moist; Loose consistence;
	 20-50%, medium gravelly, 6-20mm, subrounded, , coarse fragments; 20-50%, fine gravelly, 2-6mm, 
	subrounded, , coarse fragments; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Clear change to -
	 
	B21	0.35 - 0.65 m	Yellowish brown (10YR5/6-Moist); Mottles, 2.5YR46, 2-10% , 5-15mm, Distinct; Clay loam, sandy; Weak 
	grade of structure; Rough-ped fabric; Moist; Very weak consistence; 20-50%, medium gravelly, 6-20mm, 
	subangular, , coarse fragments; 20-50%, fine gravelly, 2-6mm, subangular, , coarse fragments; Many 
	(20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7 (Raupach); Common, very fine (0-
	1mm) roots; Clear change to - 
	B22	0.65 - 0.8 m	Strong brown (7.5YR5/6-Moist); Mottles, 2.5YR46, 10-20% , 5-15mm, Distinct; Clay loam, coarse sandy;
	 Massive grade of structure; Moist; Weak consistence; 20-50%, medium gravelly, 6-20mm, subangular, , 
	coarse fragments; 20-50%, fine gravelly, 2-6mm, subangular, , coarse fragments; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; Abrupt 
	change to - 
	B3	0.8 - 1.05 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5YR46, 20-50% , 15-30mm, Prominent; Light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Weak consistence; 20-50%, fine 
	gravelly, 2-6mm, subrounded, , coarse fragments; Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), 
	Nodules; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	B22	Very slight dispersion.         
	Observation Notes
	Site Notes
	Stanley Road.    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	0902	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.6B
	0.15 - 0.25	4.9B
	0.35 - 0.55	5.9B	5B	1.84A	1.5	0.22	0.23	3.79D
	6.7H
	0.35 - 0.55	5.9B	5B	1.84A	1.5	0.22	0.23	3.79D
	6.7H
	0.35 - 0.55	5.9B	5B	1.84A	1.5	0.22	0.23	3.79D
	6.7H
	0.4 - 0.5	5.8B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.35 - 0.55	68.5I	3.5	28
	0.35 - 0.55	68.5I	3.5	28
	0.35 - 0.55	68.5I	3.5	28
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded