Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1077	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	28/07/93	Elevation:	272 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6320150 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	540140  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	30 metres
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	225 degrees
	Surface Soil Condition 	Recently cultivated
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dg4.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	20-50%, medium gravelly, 6-20mm, angular, Quartz; No surface coarse fragments
	Profile 
	A1p	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sand; Single grain grade of structure; Moderately moist; Loose 
	consistence; Field pH 5.5 (Raupach); Many, very fine (0-1mm) roots; Abrupt change to - 
	A21	0.1 - 0.25 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; Moist; Loose
	 consistence; Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Clear change to - 
	A22e	0.25 - 0.3 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Clayey coarse sand; Single grain grade of structure; 
	Moist; Loose consistence; Field pH 7 (Raupach); Few, very fine (0-1mm) roots; Abrupt, Wavy change to - 
	B21	0.3 - 0.55 m	Light grey (10YR7/1-Moist); Mottles, 10YR56, 10-20% , 5-15mm, Distinct; Sandy light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Firm consistence; Field pH 8 
	(Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	B22	0.55 - 0.8 m	Light brownish grey (10YR6/2-Moist); Mottles, 2.5YR46, 20-50% , 15-30mm, Distinct; Medium clay; 
	Moderate grade of structure; Rough-ped fabric; Dry; Very firm consistence; Field pH 7.5 (Raupach); 
	Few, very fine (0-1mm) roots; Gradual change to - 
	B3	0.8 - 1 m	Light brownish grey (2.5Y6/3-Moist); Mottles, 10YR56, 2-10% , 5-15mm, Faint; Light medium clay; Dry; 
	Firm consistence; Field pH 7.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	Site along Dongolocking Road - slop 1% above site and >1% below site.    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1077	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.5B
	0.15 - 0.25	5.6B
	0.3 - 0.55	6.3B	6B	0.93A	1.19	0.02	0.54	2.68D
	7.6H
	0.3 - 0.55	6.3B	6B	0.93A	1.19	0.02	0.54	2.68D
	7.6H
	0.4 - 0.5	6.3B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.3 - 0.55	72.5I	8.5	19
	0.3 - 0.55	72.5I	8.5	19
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded