Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1198	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	23/08/93	Elevation:	286 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6344030 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	530190  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	2 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dg4.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; No surface coarse fragments
	Profile 
	Ap	0 - 0.12 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moderately moist; 
	Field pH 6 (Raupach); Abrupt change to - 
	A21	0.12 - 0.4 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Field pH 
	5.5 (Raupach); Clear change to - 
	A22e	0.4 - 0.45 m	Very pale brown (10YR7/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Wet; Field pH 5.5 
	(Raupach); Clear, Wavy change to - 
	B21	0.45 - 0.7 m	Light grey (10YR7/2-Moist); Mottles, 2.5YR46, 20-50% , 15-30mm, Prominent; Sandy clay loam; Weak 
	grade of structure; Rough-ped fabric; Moderately moist; Field pH 5.5 (Raupach); Clear change to - 
	B22	0.7 - 0.85 m	Light grey (10YR7/2-Moist); , 7.5YR56, 20-50% , 15-30mm, Distinct; , 2.5YR40, 10-20% , 15-30mm, 
	Prominent; Coarse sandy light medium clay; Weak grade of structure; Rough-ped fabric; Moderately 
	moist; Field pH 5.5 (Raupach); Clear change to - 
	C	0.85 - 0.9 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Coarse sandy clay loam; Massive grade of structure; 
	Moderately moist; Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site along Highbury East Road.    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	1198	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.7B
	0.15 - 0.25	4.5B
	0.4 - 0.45	4.5B
	0.45 - 0.7	4.5B	43B	0.43H	2.36	0.15	1.2	0.07J	4.14D
	5.2H
	0.45 - 0.7	4.5B	43B	0.43H	2.36	0.15	1.2	0.07J	4.14D
	5.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.4 - 0.45
	0.45 - 0.7	71.5I	5	23.5
	0.45 - 0.7	71.5I	5	23.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded