Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2313	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	28/02/95	Elevation:	330 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6265130 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	542660  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	20 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition 	Surface flake
	Erosion:	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse 	No surface coarse fragments; 20-50%, , rounded, Dolerite
	Profile 
	A1	0 - 0.1 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Sandy (grains prominent) fabric; Dry; 10-20%, fine gravelly, 2-6mm, subangular, Dolerite, coarse 
	fragments; Field pH 5.5 (Raupach); Clear change to - 
	A21	0.1 - 0.2 m	Dark reddish brown (2.5YR3/4-Moist); , 0-0% ; Clayey sand; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Dry; 10-20%, fine gravelly, 2-6mm, subangular, Dolerite, coarse 
	fragments; 10-20%, medium gravelly, 6-20mm, subangular, Dolerite, coarse fragments; Field pH 6 
	(Raupach); Gradual change to - 
	A22	0.2 - 0.3 m	Reddish brown (5YR5/4-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Dry; 10-20%, fine 
	gravelly, 2-6mm, subangular, Dolerite, coarse fragments; Field pH 6.5 (Raupach); Abrupt change to - 
	B2	0.3 - 0.6 m	Red (2.5YR4/6-Moist); , 0-0% ; Medium clay; Strong grade of structure, 50-100 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; Field pH 7 (Raupach); Clear change to - 
	B3	0.6 - 0.9 m	Strong brown (7.5YR4/6-Moist); , 2.5YR46, 2-10% , 15-30mm, Distinct; Clay loam, sandy; Moderate 
	grade of structure, 20-50 mm, Polyhedral; Smooth-ped fabric; Dry; 20-50%, medium gravelly, 6-20mm, 
	rounded, Dolerite, coarse fragments; Field pH 7.5 (Raupach); Clear change to - 
	C	0.9 - 1.2 m	Strong brown (7.5YR4/6-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Dry; Field pH 7.5 
	(Raupach); 
	Morphological Notes
	A21	Dolerite boulders and stones present         
	C	Weathered dolerite         
	Observation Notes
	Site Notes
	Soil pit on Bronte Rundle's farm "Ucarro" CSIRO soil pit    

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2313	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.7B	10B	6.5H	1.2	0.59	0.13	0.22J	8.42D
	5.5H	11B
	4.7B
	4.8B
	5.4H
	0 - 0.1	4.7B	10B	6.5H	1.2	0.59	0.13	0.22J	8.42D
	5.5H	11B
	4.7B
	4.8B
	5.4H
	0 - 0.1	4.7B	10B	6.5H	1.2	0.59	0.13	0.22J	8.42D
	5.5H	11B
	4.7B
	4.8B
	5.4H
	0 - 0.1	4.7B	10B	6.5H	1.2	0.59	0.13	0.22J	8.42D
	5.5H	11B
	4.7B
	4.8B
	5.4H
	0 - 0.1	4.7B	10B	6.5H	1.2	0.59	0.13	0.22J	8.42D
	5.5H	11B
	4.7B
	4.8B
	5.4H
	0.1 - 0.2	4.9B	4B	5.5H	1.2	0.31	0.13	0.12J	7.14D
	5.9H
	4.9B
	0.1 - 0.2	4.9B	4B	5.5H	1.2	0.31	0.13	0.12J	7.14D
	5.9H
	4.9B
	0.1 - 0.2	4.9B	4B	5.5H	1.2	0.31	0.13	0.12J	7.14D
	5.9H
	4.9B
	0.2 - 0.3	6B	4B	7.7A	7.7	0.26	0.68	16.34D
	7.4H
	0.2 - 0.3	6B	4B	7.7A	7.7	0.26	0.68	16.34D
	7.4H
	0.3 - 0.6	6B	4B	7.8A	7.9	0.25	0.66	16.61D
	7.3H
	0.3 - 0.5	6.3B	6B	7.6A	7.7	0.26	0.63	16.19D
	7.4H
	0.3 - 0.6	6B	4B	7.8A	7.9	0.25	0.66	16.61D
	7.3H
	0.3 - 0.5	6.3B	6B	7.6A	7.7	0.26	0.63	16.19D
	7.4H
	0.4 - 0.5	6.4B
	0.6 - 0.9	6.6B	10B	14A	19	0.21	2.7	35.91D
	7.7H
	0.6 - 0.9	6.6B	10B	14A	19	0.21	2.7	35.91D
	7.7H

	Project Name:	Katanning land resources survey
	Project Code:	KLC	Site ID:	2313	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.9 - 1.2	6.8B	6B	12E	15	0.15	3.4	30B	30.55D	11.33
	8.3H
	0.9 - 1.2	6.8B	6B	12E	15	0.15	3.4	30B	30.55D	11.33
	8.3H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.68D	230B	0.164E	10.9	9
	2D	260B	0.185E
	0 - 0.1	1.68D	230B	0.164E	10.9	9
	2D	260B	0.185E
	0 - 0.1	1.68D	230B	0.164E	10.9	9
	2D	260B	0.185E
	0 - 0.1	1.68D	230B	0.164E	10.9	9
	2D	260B	0.185E
	0 - 0.1	1.68D	230B	0.164E	10.9	9
	2D	260B	0.185E
	0.1 - 0.2	0.74D	120B	0.078E	10.4	10.5
	0.1 - 0.2	0.74D	120B	0.078E	10.4	10.5
	0.1 - 0.2	0.74D	120B	0.078E	10.4	10.5
	0.2 - 0.3	0.35D	69B	0.047E	10.6	28.9
	0.2 - 0.3	0.35D	69B	0.047E	10.6	28.9
	0.3 - 0.6	0.34D	61B	0.038E	10.4	29.9
	0.3 - 0.5	0.37D	61B	0.053E	10	49.5
	0.3 - 0.6	0.34D	61B	0.038E	10.4	29.9
	0.3 - 0.5	0.37D	61B	0.053E	10	49.5
	0.4 - 0.5
	0.6 - 0.9	0.1D	83B	0.012E	13.6	25.9
	0.6 - 0.9	0.1D	83B	0.012E	13.6	25.9
	0.9 - 1.2	<2C	0.05D	63B	0.006E	10.2	20.1
	0.9 - 1.2	<2C	0.05D	63B	0.006E	10.2	20.1
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)