Project Name:	Knox Creek Plain survey (Kununurra)
	Project Code:	KNX	Site ID:	0138	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Noel Schoknecht	Locality:
	Date Desc.:	13/06/94	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	8272582 AMG zone: 52	Runoff:	No Data
	Easting/Lat.:	497263  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse 
	Profile 
	A11	0 - 0.06 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, Granular; 
	Rough-ped fabric; Dry; Firm consistence; Field pH 6.9 (pH meter); Clear change to - 
	A12	0.06 - 0.25 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, 
	Subangular blocky; Rough-ped fabric; Dry; Very firm consistence; Very few (0 - 2 %), Manganiferous, 
	Fine (0 - 2 mm), Concretions; Field pH 7.1 (pH meter); Gradual change to - 
	B21	0.25 - 1.02 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Weak grade of structure, 50-100 mm, 
	Prismatic; Smooth-ped fabric; Moderately moist; Strong consistence; Very few (0 - 2 %), Manganiferous,
	 Fine (0 - 2 mm), Concretions; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Concretions; Field pH 
	8.1 (pH meter); Clear change to - 
	B22	1.02 - 1.8 m	Brown (7.5YR4/3-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, Angular blocky; 
	Smooth-ped fabric; Moist; Strong consistence; Few (2 - 10 %), Gypseous, Medium (2 -6 mm), Crystals; 
	Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Concretions; Field pH 8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site is gilgaied with 5mm crust and prominent cracks which extend to 60cms. Main roots to 75cms and fine to 150. Primary structure of 
	layers3-5 - 5ABS. PEDAL GREY VERTOSOL Sampled: 0-6; 6-25; 25-72; 75-102; 102-180.

	Project Name:	Knox Creek Plain survey (Kununurra)
	Project Code:	KNX	Site ID:	0138	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.1B	23B	12.08A	13.99	1.2	0.33	27.6D
	6.6H
	0.06 - 0.25	6.4B	31B	15.1A	14.32	0.91	0.63	30.96D
	6.8H
	0.25 - 0.72	7.2B	87B	18.59A	14.33	0.98	1.75	35.65D
	7.6H
	0.72 - 1.02	7.9B	150B	15.57E	12.95	0.42	3.86	29B	32.8D	13.31
	8.2H
	1.02 - 1.8	7.8B	430B	11.18E	17.1	0.46	7.02	29B	35.76D	24.21
	7.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	0.63D	60B	0.039E	13.8	46.2
	0.06 - 0.25	0.33D	40B	0.021E	13.4	50.5
	0.25 - 0.72	0.3D	46B	0.018E	13.9	48.7
	0.72 - 1.02	2C	0.3D	40B	0.019E	14.1	50.3
	1.02 - 1.8	0.13D	36B	0.01E	12.5	47.5
	Laboratory Analyses Completed for this profile
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct

	Project Name:	Knox Creek Plain survey (Kununurra)
	Project Code:	KNX	Site ID:	0138	Observation 	1
	Agency Name:	Agriculture Western Australia
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)