Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	1189	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Mir Frahmand	Locality:
	Date Desc.:	18/03/96	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6565166 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	438784  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	0 degrees
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Sequi-Nodular Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Clayey fine sand; Massive grade of structure; Moderately moist; 2-
	10%, rounded, Ironstone, coarse fragments; Field pH 7.1 (pH meter); Clear, Wavy change to - 
	A2	0.1 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Clayey fine sand; Massive grade of structure; Moist; 2-10%, rounded, 
	Ironstone, coarse fragments; Field pH 7.1 (pH meter); Abrupt, Smooth change to - 
	B21ec	0.3 - 0.55 m	Very pale brown (10YR7/3-Moist); ; Clayey fine sand; , Granular; Dry; 50-90%, rounded, Ironstone, 
	coarse fragments; Field pH 7.1 (pH meter); Diffuse, Wavy change to - 
	B2c	0.55 - 0.9 m	Light yellowish brown (10YR6/4-Moist); ; Massive grade of structure; Dry; 50-90%, rounded, Ironstone, 
	coarse fragments; Field pH 7 (pH meter); Clear, Smooth change to - 
	B2c	0.9 - 1.2 m	Brownish yellow (10YR6/6-Moist); , 2.5YR36, 20-50% , Distinct; , 10YR72, 2-10% , Distinct; Sandy loam;
	 Massive grade of structure; Moist; 20-50%, angular, Ironstone, coarse fragments; 2-10%, rounded, 
	Ironstone, coarse fragments; Very many (50 - 100 %), Ferruginous, Fine (0 - 2 mm), Soft segregations; ,
	 Ferruginous, Medium (2 -6 mm), Soft segregations; Field pH 6.5 (pH meter); Clear, Smooth change to 
	- 
	B3	1.2 - 2 m	Brownish yellow (10YR6/8-Moist); , 2.5YR20, 2-10% , Faint; Sandy loam; Massive grade of structure; 
	Moist; Field pH 6.2 (pH meter); 
	Morphological Notes
	A2	fvwls
	Observation Notes
	Site Notes
	Bown sandy earth

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	1189	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.8B	10B	2.85A	0.79	0.16	0.04	3.84D
	7.4H
	0.1 - 0.3	6.6B	6B	1.88A	0.65	0.18	0.02	2.73D
	7.3H
	0.3 - 0.55	5.4B	3B	0.55A	0.24	0.4	0.04	1.23D
	6.7H
	0.55 - 0.9	5.9B	4B	1.3A	0.45	0.26	0.15	2.16D
	7H
	0.9 - 1.2	6.2B	7B	1.67A	0.82	0.05	0.28	2.82D
	6.8H
	1.2 - 2	6.3B	10B	1.54A	1.12	0.04	0.24	2.94D
	6.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.94D	110B	0.078E	0.6	1.8
	0.1 - 0.3	0.6D	0.8	4
	0.3 - 0.55	0.14D	0.8	10.2
	0.55 - 0.9	0.16D	1.1	15.7
	0.9 - 1.2	0.11D	1.2	12
	1.2 - 2	0.1D	2.8	11.2
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)

	Project Name:	Moora Wongan Hills land resources survey
	Project Code:	MRA	Site ID:	1189	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)