Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0357	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Noel Schoknecht	Locality:
	Date Desc.:	09/05/92	Elevation:	180 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6644720 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	350960  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Petroferric Bleached-Orthic Tenosol     	Principal Profile Form:	Uc4.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.15 m	Greyish brown (10YR5/2-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; Water repellent; Field pH 6.5 (pH meter); Clear, Wavy 
	change to - 
	A21	0.15 - 0.23 m	Pale brown (10YR6/3-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Field pH 6.5 (pH meter); Abrupt, Wavy change to - 
	A22	0.23 - 0.65 m	Pale brown (10YR6/3-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Moist; 50-90%, Granulite, coarse fragments; Water repellent; Field pH 6.5 (pH meter); Gradual, 
	Wavy change to - 
	2B2w	0.65 - 0.9 m	Reddish yellow (7.5YR7/8-Moist); , 10YR76, 10-20% , 5-15mm, Faint; , 5YR58, 10-20% , 5-15mm, 
	Distinct; Loamy sand; Moderate grade of structure; Moist; 50-90%, Granulite, coarse fragments; Field 
	pH 6.5 (pH meter); Gradual, Wavy change to - 
	2C	0.9 - 1.15 m	Yellow (10YR7/6-Moist); , 7.5YR68, 20-50% , 5-15mm, Distinct; Clayey sand; Moderate grade of 
	structure; Moist; Field pH 6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Site is located on the upper slope of a lateritic remnant hill. ORIGINALLY SITE 60 Slope - 2% along ridge and 5-6% across ridge. Basic 
	petroferric nodular tenosol.

	Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0357	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5B	4B	1.55H	0.26	0.08	0.03	<0.02J	1.92D
	5.8H	4.3B
	5.6H
	0 - 0.15	5B	4B	1.55H	0.26	0.08	0.03	<0.02J	1.92D
	5.8H	4.3B
	5.6H
	0 - 0.15	5B	4B	1.55H	0.26	0.08	0.03	<0.02J	1.92D
	5.8H	4.3B
	5.6H
	0.15 - 0.23	4.8B	5B	1.84H	0.36	0.03	0.07	0.06J	2.3D
	5.6H	4.4B
	5.3H
	0.15 - 0.23	4.8B	5B	1.84H	0.36	0.03	0.07	0.06J	2.3D
	5.6H	4.4B
	5.3H
	0.15 - 0.23	4.8B	5B	1.84H	0.36	0.03	0.07	0.06J	2.3D
	5.6H	4.4B
	5.3H
	0.23 - 0.65	5B	3B	0.87H	0.3	0.06	0.04	0.05J	1.27D
	5.7H	3.3B
	5.4H
	0.23 - 0.65	5B	3B	0.87H	0.3	0.06	0.04	0.05J	1.27D
	5.7H	3.3B
	5.4H
	0.23 - 0.65	5B	3B	0.87H	0.3	0.06	0.04	0.05J	1.27D
	5.7H	3.3B
	5.4H
	0.65 - 0.9	5B	3B	0.71H	0.33	0.19	0.09	0.05J	1.32D
	6H	3.3B
	5.7H
	0.65 - 0.9	5B	3B	0.71H	0.33	0.19	0.09	0.05J	1.32D
	6H	3.3B
	5.7H
	0.65 - 0.9	5B	3B	0.71H	0.33	0.19	0.09	0.05J	1.32D
	6H	3.3B
	5.7H
	0.9 - 1.15	4.8B	3B	0.52H	0.39	0.15	0.09	0.05J	1.15D
	5.9H
	5.4H
	0.9 - 1.15	4.8B	3B	0.52H	0.39	0.15	0.09	0.05J	1.15D
	5.9H
	5.4H
	0.9 - 1.15	4.8B	3B	0.52H	0.39	0.15	0.09	0.05J	1.15D
	5.9H
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	0.72D	42B	0.044E	0.6	1.5

	Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0357	Observation 	1
	Agency Name:	Agriculture Western Australia
	0 - 0.15	0.72D	42B	0.044E	0.6	1.5
	0 - 0.15	0.72D	42B	0.044E	0.6	1.5
	0.15 - 0.23	0.88D	38B	0.036E	1.8	4.8
	0.15 - 0.23	0.88D	38B	0.036E	1.8	4.8
	0.15 - 0.23	0.88D	38B	0.036E	1.8	4.8
	0.23 - 0.65	0.48D	35B	0.025E	1.7	5.3
	0.23 - 0.65	0.48D	35B	0.025E	1.7	5.3
	0.23 - 0.65	0.48D	35B	0.025E	1.7	5.3
	0.65 - 0.9	24B	0.015E	2.2	14.5
	0.65 - 0.9	24B	0.015E	2.2	14.5
	0.65 - 0.9	24B	0.015E	2.2	14.5
	0.9 - 1.15	19B	0.008E	2.4	19.7
	0.9 - 1.15	19B	0.008E	2.4	19.7
	0.9 - 1.15	19B	0.008E	2.4	19.7
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)