Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0876	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Noel Schoknecht	Locality:
	Date Desc.:	10/12/92	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6633384 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	329019  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Grey Sodosol Very thick Non-	Principal Profile Form:	Dy5.83
	gravelly Sandy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; Very 
	weak consistence; Strongly water repellent, "Field pH 6.5 (pH meter); Clear, Wavy change to - 
	A21	0.1 - 0.35 m	Light grey (10YR7/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; Very weak 
	consistence; Field pH 7 (pH meter); Diffuse change to - 
	A22	0.35 - 0.68 m	Very pale brown (10YR7/3-Moist); , 10YR58, 2-10% , 0-5mm, Faint; Clayey sand; Single grain grade of 
	structure; Moist; Very weak consistence; Field pH 9 (pH meter); Sharp, Smooth change to - 
	B21	0.68 - 0.9 m	Light grey (10YR7/1-Moist); , 10YR58, 10-20% , 5-15mm, Prominent; Medium clay; Weak grade of 
	structure, 20-50 mm, Columnar; Rough-ped fabric; Moist; Very firm consistence; Field pH 9 (pH meter); 
	Diffuse change to - 
	B21	0.9 - 1.25 m	Light grey (10YR7/1-Moist); , 10YR58, 20-50% , 5-15mm, Prominent; , 5G42, 2-10% , 0-5mm, Distinct; 
	Light medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; Rough-ped fabric; Moist; 
	Very firm consistence; Field pH 9 (pH meter); Diffuse change to - 
	B23	1.25 - 1.7 m	Light grey (10YR7/1-Moist); , 10YR76, 2-10% , 15-30mm, Distinct; Sandy light clay; Moderate grade of 
	structure; Moist; Firm consistence; Field pH 9 (pH meter); 
	Morphological Notes
	A22	bound - smooth and continuous
	B21	Red surfaces(columns) 10YR 5/2.
	Observation Notes
	Site Notes
	Moderately deep mottled duplex soil.

	Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0876	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.6B	22B	1.26H	0.64	0.06	0.44	0.03J	2.4D
	6.4H	21.5B
	6.3H
	0 - 0.1	5.6B	22B	1.26H	0.64	0.06	0.44	0.03J	2.4D
	6.4H	21.5B
	6.3H
	0 - 0.1	5.6B	22B	1.26H	0.64	0.06	0.44	0.03J	2.4D
	6.4H	21.5B
	6.3H
	0.1 - 0.35	6.4B	8B	1.08A	0.17	<0.02	0.26	1.52D
	7.1H	8.4B
	6.8H
	0.1 - 0.35	6.4B	8B	1.08A	0.17	<0.02	0.26	1.52D
	7.1H	8.4B
	6.8H
	0.1 - 0.35	6.4B	8B	1.08A	0.17	<0.02	0.26	1.52D
	7.1H	8.4B
	6.8H
	0.35 - 0.68	7.3B	33B	0.25E	0.27	<0.02	0.16	1B	0.69D	16.00
	7.9H	30.7B
	8H
	0.35 - 0.68	7.3B	33B	0.25E	0.27	<0.02	0.16	1B	0.69D	16.00
	7.9H	30.7B
	8H
	0.35 - 0.68	7.3B	33B	0.25E	0.27	<0.02	0.16	1B	0.69D	16.00
	7.9H	30.7B
	8H
	0.68 - 0.9	7.2B	57B	2.44E	3.93	0.3	2.89	11B	9.56D	26.27
	8.1H	55.2B
	7.9H
	0.68 - 0.9	7.2B	57B	2.44E	3.93	0.3	2.89	11B	9.56D	26.27
	8.1H	55.2B
	7.9H
	0.68 - 0.9	7.2B	57B	2.44E	3.93	0.3	2.89	11B	9.56D	26.27
	8.1H	55.2B
	7.9H
	0.9 - 1.25	7.3B	51B	2.7E	4.72	0.34	4.01	11B	11.77D	36.45
	8.3H	49.2B
	8.1H
	0.9 - 1.25	7.3B	51B	2.7E	4.72	0.34	4.01	11B	11.77D	36.45
	8.3H	49.2B
	8.1H
	0.9 - 1.25	7.3B	51B	2.7E	4.72	0.34	4.01	11B	11.77D	36.45
	8.3H	49.2B
	8.1H
	1.25 - 1.7	7.4B	60B	1.48E	3.11	0.16	1.86	7B	6.61D	26.57
	8.2H	58.1B
	8H
	1.25 - 1.7	7.4B	60B	1.48E	3.11	0.16	1.86	7B	6.61D	26.57
	8.2H	58.1B
	8H

	Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0876	Observation 	1
	Agency Name:	Agriculture Western Australia
	1.25 - 1.7	7.4B	60B	1.48E	3.11	0.16	1.86	7B	6.61D	26.57
	8.2H	58.1B
	8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.5D	48B	0.031E	1.7	1.4
	0 - 0.1	0.5D	48B	0.031E	1.7	1.4
	0 - 0.1	0.5D	48B	0.031E	1.7	1.4
	0.1 - 0.35	0.08D	14B	0.003E	1	0.6
	0.1 - 0.35	0.08D	14B	0.003E	1	0.6
	0.1 - 0.35	0.08D	14B	0.003E	1	0.6
	0.35 - 0.68	<2C	0.07D	19B	0.004E	1.2	1.4
	0.35 - 0.68	<2C	0.07D	19B	0.004E	1.2	1.4
	0.35 - 0.68	<2C	0.07D	19B	0.004E	1.2	1.4
	0.68 - 0.9	<2C	25B	0.011E	1.2	48.1
	0.68 - 0.9	<2C	25B	0.011E	1.2	48.1
	0.68 - 0.9	<2C	25B	0.011E	1.2	48.1
	0.9 - 1.25	<2C	22B	0.005E	6.9	17.5
	0.9 - 1.25	<2C	22B	0.005E	6.9	17.5
	0.9 - 1.25	<2C	22B	0.005E	6.9	17.5
	1.25 - 1.7	21B	0.003E	0.1	36.3
	1.25 - 1.7	21B	0.003E	0.1	36.3
	1.25 - 1.7	21B	0.003E	0.1	36.3
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC

	Project Name:	North Coastal Plain land resources survey
	Project Code:	NCP	Site ID:	0876	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)