Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0111	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	07/06/95	Elevation:	350 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6277490 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	627740  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	5 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Natric Brown Kurosol     	Principal Profile Form:	Db2.11
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , angular, Quartz
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Sandy (grains prominent) fabric; Dry; Field pH 6 (Raupach); Abundant, very fine (0-
	1mm) roots; Abrupt change to - 
	B21	0.08 - 0.2 m	Dark yellowish brown (10YR4/4-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; Rough-
	ped fabric; Dry; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	B22	0.2 - 0.4 m	Pale brown (10YR6/3-Moist); Mottles, 5YR56, 10-20% , 5-15mm, Distinct; Medium clay; Strong grade of
	 structure; Rough-ped fabric; Dry; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Abrupt change 
	to - 
	B3	0.4 - 0.5 m	Light grey (10YR7/2-Moist); Mottles, 5YR56, 10-20% , 15-30mm, Distinct; Light medium clay; Strong 
	grade of structure; Smooth-ped fabric; Dry; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	 Site downslope of an indistinct breakaway - "Hardsetting grey clay".

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0111	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.08 - 0.28	4.1B	37B	0.59H	4.17	0.19	1.85	1.94J	6.8D
	4.8H
	0.08 - 0.28	4.1B	37B	0.59H	4.17	0.19	1.85	1.94J	6.8D
	4.8H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.08 - 0.28	38I	2.5	59.5
	0.08 - 0.28	38I	2.5	59.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded