Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0112	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	08/06/95	Elevation:	330 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6273030 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	609340  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	20 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	90 degrees
	Surface Soil Condition 	Firm
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Mesonatric Brown Sodosol     	Principal Profile Form:	Dy5.62
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subrounded, ; 0-2%, , subrounded, 
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Field pH 6 
	(Raupach); Abrupt, Wavy change to - 
	A21	0.1 - 0.3 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Clayey sand; Single grain grade of structure; Wet; 10-
	20%, fine gravelly, 2-6mm, rounded, , coarse fragments; Field pH 6.5 (Raupach); Abrupt change to - 
	A22c	0.3 - 0.4 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Single grain grade of structure; Wet; 20-50%, fine 
	gravelly, 2-6mm, subrounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, subrounded, , 
	coarse fragments; Field pH 7 (Raupach); Abrupt change to - 
	B21c	0.4 - 0.5 m	Yellowish brown (10YR5/6-Moist); Mottles, 2.5YR46, 2-10% , 5-15mm, Distinct; Clay loam, sandy; 
	Massive grade of structure; Moderately moist; Field pH 7 (Raupach); 
	B22	0.5 - 0.8 m	Strong brown (7.5YR5/6-Moist); Mottles, 2.5YR46, 10-20% , 0-5mm, Distinct; Clay loam, sandy; Massive
	 grade of structure; Dry; Field pH 7 (Raupach); Gradual change to - 
	B3	0.8 - 0.9 m	Strong brown (7.5YR5/6-Moist); Mottles, 10YR73, 2-10% , 15-30mm, Distinct; , 2.5YR46, 10-20% , 5-
	15mm, Distinct; Light medium clay; Weak grade of structure; Dry; Field pH 8 (Raupach); 
	Morphological Notes
	A21	Medium to coarse sand.         
	A22c	Medium to coarse sand.         
	B21c	> 20% gravel - very slight dispersion.         
	B3	Very slight dispersion.         
	Observation Notes
	Site Notes

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0112	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.7B
	0.15 - 0.25	4.6B
	0.4 - 0.6	5.9B	14B	0.96A	2.66	0.06	0.91	4.59D
	6.5H	0.96A	2.66	0.06	0.91	4.59D
	5.9B
	6.5H
	0.4 - 0.6	5.9B	14B	0.96A	2.66	0.06	0.91	4.59D
	6.5H	0.96A	2.66	0.06	0.91	4.59D
	5.9B
	6.5H
	0.4 - 0.5	5.8B
	0.4 - 0.6	5.9B	14B	0.96A	2.66	0.06	0.91	4.59D
	6.5H	0.96A	2.66	0.06	0.91	4.59D
	5.9B
	6.5H
	0.4 - 0.6	5.9B	14B	0.96A	2.66	0.06	0.91	4.59D
	6.5H	0.96A	2.66	0.06	0.91	4.59D
	5.9B
	6.5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.4 - 0.6	62I	5.5	32.5
	62I	5.5	32.5
	0.4 - 0.6	62I	5.5	32.5
	62I	5.5	32.5
	0.4 - 0.5
	0.4 - 0.6	62I	5.5	32.5
	62I	5.5	32.5
	0.4 - 0.6	62I	5.5	32.5
	62I	5.5	32.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0112	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded