Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0125	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	13/06/95	Elevation:	300 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6268760 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	605250  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	5 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesonatric Yellow Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subrounded, ; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Wet; Loose 
	consistence; 10-20%, medium gravelly, 6-20mm, subrounded, , coarse fragments; Field pH 5.5 
	(Raupach); Abrupt change to - 
	A21e	0.1 - 0.3 m	Pale brown (10YR6/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Wet; Loose consistence; 
	10-20%, fine gravelly, 2-6mm, subrounded, , coarse fragments; 20-50%, medium gravelly, 6-20mm, 
	subrounded, , coarse fragments; Field pH 6 (Raupach); 
	A22ec	0.3 - 0.5 m	Pale brown (10YR6/3-Moist); , 0-0% ; Single grain grade of structure; Wet; Loose consistence; 10-20%, 
	fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 20-50%, fine gravelly, 2-6mm, subrounded, ,
	 coarse fragments; 20-50%, medium gravelly, 6-20mm, subrounded, , coarse fragments; Field pH 6.5 
	(Raupach); Clear, Wavy change to - 
	B2t	0.5 - 0.75 m	Brownish yellow (10YR6/6-Moist); Mottles, 2.5Y73, 10-20% , 5-15mm, Faint; Light medium clay; Weak 
	grade of structure; Rough-ped fabric; Dry; 10-20%, fine gravelly, 2-6mm, subrounded, , coarse 
	fragments; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 8 (Raupach); 
	Morphological Notes
	A22ec	Coarse sand(KS).
	B2t	pH 8.5 at 70cm.         
	Observation Notes
	Site Notes
	Site in cereal stubble.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0125	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.3B	8B
	5.1H
	0.15 - 0.25	4.3B	1B
	5.2H
	0.35 - 0.45	5.7B	2B
	6.6H
	0.5 - 0.7	6.6B	9B	2.37A	4.1	0.21	1.53	8.21D
	7.9H
	0.5 - 0.7	6.6B	9B	2.37A	4.1	0.21	1.53	8.21D
	7.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.25
	0.35 - 0.45
	0.5 - 0.7	34.5I	4	61.5
	0.5 - 0.7	34.5I	4	61.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded