Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0134	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	14/06/95	Elevation:	330 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6275960 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	609310  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	5 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition 	Cracking, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Episodic Epipedal Red Vertosol     	Principal Profile Form:	Ug5.37
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Clay loam; Strong grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Wet; Field pH 7 (Raupach); Abrupt, Wavy change to - 
	B1	0.03 - 0.15 m	Red (2.5YR4/6-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; Rough-ped fabric; Wet; 
	Field pH 7 (Raupach); Clear change to - 
	B2	0.15 - 0.55 m	Dark reddish brown (2.5YR3/4-Moist); , 0-0% ; Medium clay; Strong grade of structure; Smooth-ped 
	fabric; Moderately moist; Common cutans, 10-50% of ped faces or walls coated; Field pH 6 (Raupach); 
	B3	0.55 - 0.75 m	Yellowish red (5YR4/6-Moist); Substrate influence, 10YR58, 10-20% , 30-mm, Distinct; Medium clay; 
	Strong grade of structure; Smooth-ped fabric; Moderately moist; Field pH 6 (Raupach); 
	c	0.75 - 0.9 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Clay loam; Massive grade of structure; Field pH 5.5 
	(Raupach); 
	Morphological Notes
	A1	Too wet to texture accurately.
	c	Weathered dolerite
	Observation Notes
	Site Notes
	Cultivated paddocks have shallow clay - hardsetting grey clay with dolerite dykes cutting through the paddock.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0134	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.15	6.6B	20B	4.48A	11.31	0.63	2.72	19.14D
	7.7H
	0.03 - 0.15	6.6B	20B	4.48A	11.31	0.63	2.72	19.14D
	7.7H
	0.15 - 0.55	5.7B	39B	2.84A	9.84	0.55	4.37	17.6D
	6.6H
	0.15 - 0.55	5.7B	39B	2.84A	9.84	0.55	4.37	17.6D
	6.6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.15	41I	14	45
	0.03 - 0.15	41I	14	45
	0.15 - 0.55	35I	15.5	49.5
	0.15 - 0.55	35I	15.5	49.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded