Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0181	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	03/07/95	Elevation:	350 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6262530 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	626165  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	5 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition 	Firm
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Dystrophic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sand; Massive grade of structure; Moderately moist; Field pH 5.5 
	(Raupach); Sharp, Smooth change to - 
	A2e	0.1 - 0.2 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Moderately
	 moist; Field pH 5.5 (Raupach); 
	B21t	0.2 - 0.4 m	Pale brown (10YR6/3-Moist); Mottles, 5YR56, 20-50% , 15-30mm, Distinct; Sandy medium clay; Strong 
	grade of structure; Rough-ped fabric; Moderately moist; Field pH 6 (Raupach); Gradual, Wavy change to
	 - 
	B22t	0.4 - 0.7 m	Red (2.5YR4/6-Moist); Mottles, 10YR74, 10-20% , 5-15mm, Distinct; Medium clay; Strong grade of 
	structure; Rough-ped fabric; Moderately moist; Field pH 7 (Raupach); Gradual change to - 
	B3	0.7 - 0.8 m	Pink (7.5YR7/4-Moist); Mottles, 10YR81, 10-20% , 15-30mm, Distinct; , 2.5YR46, 2-10% , 5-15mm, 
	Distinct; Medium clay; Strong grade of structure; Smooth-ped fabric; Dry; Field pH 8.5 (Raupach); 
	Morphological Notes
	B22t	Kaolinitic clay
	B3	Kaolinitic
	Observation Notes
	Site Notes

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0181	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.2B
	0.1 - 0.2	4.1B
	0.2 - 0.4	4.5B	6B	0.63H	0.83	0.03	0.38	0.35J	1.87D
	5.9H
	0.2 - 0.4	4.5B	6B	0.63H	0.83	0.03	0.38	0.35J	1.87D
	5.9H
	0.4 - 0.5	5.2B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4	0.34D	55.5I	3	41.5
	0.2 - 0.4	0.34D	55.5I	3	41.5
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded