Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0244	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	17/07/95	Elevation:	310 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6252180 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	603550  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	10 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dy3.11
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	2-10%, medium gravelly, 6-20mm, subangular, Quartz; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); ; Sand; Massive grade of structure; Moist; Field pH 5.5 (Raupach); Abrupt, 
	Wavy change to - 
	B21	0.1 - 0.4 m	Light brownish grey (2.5Y6/3-Moist); Mottles, 5YR56, 10-20% , 5-15mm, Distinct; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Field pH 6 (Raupach); Clear change 
	to - 
	B22	0.4 - 0.6 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 5YR56, 2-10% , 5-15mm, Faint; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Dry; Field pH 6 (Raupach); 
	Morphological Notes
	A1	Thin light grey sandy A2 (1-2cm) sometimes present.         
	B22	Very slight dispersion.         
	Observation Notes
	Site Notes
	"Hardsetting grey clay".    Base Status of upper B2  is 15.7 (just Eutrophic)

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0244	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.7B	8B	2.1H	1.09	0.33	0.33	0.13J	3.85D
	5.8H
	0 - 0.1	4.7B	8B	2.1H	1.09	0.33	0.33	0.13J	3.85D
	5.8H
	0 - 0.1	4.7B	8B	2.1H	1.09	0.33	0.33	0.13J	3.85D
	5.8H
	0.1 - 0.3	4.9B	10B	1.36H	3.18	0.07	1.19	0.1J	5.8D
	6.2H
	0.1 - 0.3	4.9B	10B	1.36H	3.18	0.07	1.19	0.1J	5.8D
	6.2H
	0.1 - 0.3	4.9B	10B	1.36H	3.18	0.07	1.19	0.1J	5.8D
	6.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.44D	87.5I	4.5	8
	0 - 0.1	1.44D	87.5I	4.5	8
	0 - 0.1	1.44D	87.5I	4.5	8
	0.1 - 0.3	0.34D	60.5I	2.5	37
	0.1 - 0.3	0.34D	60.5I	2.5	37
	0.1 - 0.3	0.34D	60.5I	2.5	37
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded