Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0270	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	24/07/95	Elevation:	330 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6291600 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	618810  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Natric Red Kurosol     	Principal Profile Form:	Dr3.11
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , angular, Quartz
	Profile Morphology
	A1	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Clayey fine sand; Massive grade of structure; Moderately 
	moist; Field pH 6 (Raupach); Abrupt change to - 
	A3e	0.08 - 0.14 m	Pale brown (10YR6/3-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moist; Field pH 6 
	(Raupach); Abrupt, Wavy change to - 
	B2t	0.14 - 0.3 m	Reddish yellow (5YR6/6-Moist); Mottles, 2.5YR46, 2-10% , 5-15mm, Distinct; Sandy light medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Field pH 5.5 (Raupach); Gradual 
	change to - 
	B3	0.3 - 0.5 m	Red (2.5YR4/6-Moist); Mottles, 10YR72, 20-50% , 15-30mm, Distinct; Sandy medium clay; Strong grade
	 of structure; Smooth-ped fabric; Moderately moist; Field pH 5.5 (Raupach); Clear change to - 
	C	0.5 - 0.6 m	Very pale brown (10YR7/3-Moist); Mottles, 2.5YR36, 20-50% , 15-30mm, Distinct; Medium clay; Strong 
	grade of structure; Smooth-ped fabric; Moderately moist; Field pH 6 (Raupach); 
	Morphological Notes
	B3	Kaolinitic clay.         
	C	Kaolinitic clay.         
	Observation Notes
	Site Notes
	"Hardsetting grey clay" - cotula on surface - area nearby is affected by wind erosion and clay is <5cm from surface - shows white on colour 
	photographs.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0270	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.5B	13B	1.75A	0.91	0.19	0.3	3.15D
	6.6H
	0 - 0.08	5.5B	13B	1.75A	0.91	0.19	0.3	3.15D
	6.6H
	0 - 0.08	5.5B	13B	1.75A	0.91	0.19	0.3	3.15D
	6.6H
	0.14 - 0.34	4.1B	5B	0.29H	0.66	<0.02	0.31	0.64J	1.27D
	5.4H
	0.14 - 0.34	4.1B	5B	0.29H	0.66	<0.02	0.31	0.64J	1.27D
	5.4H
	0.14 - 0.34	4.1B	5B	0.29H	0.66	<0.02	0.31	0.64J	1.27D
	5.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	2.04D	88.5I	4	7.5
	0 - 0.08	2.04D	88.5I	4	7.5
	0 - 0.08	2.04D	88.5I	4	7.5
	0.14 - 0.34	0.31D	58.5I	4.5	37
	0.14 - 0.34	0.31D	58.5I	4.5	37
	0.14 - 0.34	0.31D	58.5I	4.5	37
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0270	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded