Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0282	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	25/07/95	Elevation:	340 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6289240 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	610980  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	10 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition 	Recently cultivated, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Subnatric Yellow Sodosol     	Principal Profile Form:	Dy2.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subrounded, ; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moist; 10-
	20%, medium gravelly, 6-20mm, rounded, , coarse fragments; Field pH 6 (Raupach); Abrupt, Wavy 
	change to - 
	B1	0.1 - 0.12 m	Light yellowish brown (10YR6/4-Moist); , 0-0% ; Sandy clay loam; Massive grade of structure; Moist; 
	Field pH 7.5 (Raupach); Abrupt, Wavy change to - 
	B21	0.12 - 0.5 m	Light yellowish brown (2.5Y6/4-Moist); , 0-0% ; Sandy light medium clay; Moderate grade of structure; 
	Rough-ped fabric; Moderately moist; Soil matrix is Slightly calcareous; Field pH 9 (Raupach); Gradual 
	change to - 
	B22k	0.5 - 0.7 m	Light yellowish brown (2.5Y6/4-Moist); Mottles, 10YR58, 10-20% , 5-15mm, Faint; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; 0-2%, medium gravelly, 6-20mm, 
	Calcrete, coarse fragments; Soil matrix is Slightly calcareous; Field pH 9.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	"Hardsetting grey clay".

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0282	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.5B	9B	2.76A	2	0.31	0.26	5.33D
	6.5H
	0 - 0.1	5.5B	9B	2.76A	2	0.31	0.26	5.33D
	6.5H
	0 - 0.1	5.5B	9B	2.76A	2	0.31	0.26	5.33D
	6.5H
	0.12 - 0.32	7.4B	13B	1.9E	6.07	0.14	1.78	12B	9.89D	14.83
	8.7H
	0.12 - 0.32	7.4B	13B	1.9E	6.07	0.14	1.78	12B	9.89D	14.83
	8.7H
	0.12 - 0.32	7.4B	13B	1.9E	6.07	0.14	1.78	12B	9.89D	14.83
	8.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.4D	84I	5	11
	0 - 0.1	1.4D	84I	5	11
	0 - 0.1	1.4D	84I	5	11
	0.12 - 0.32	<2C	0.17D	61I	3.5	35.5
	0.12 - 0.32	<2C	0.17D	61I	3.5	35.5
	0.12 - 0.32	<2C	0.17D	61I	3.5	35.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0282	Observation 	1
	Agency Name:	Agriculture Western Australia
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded