Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0327	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	02/08/95	Elevation:	320 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6251380 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	606565  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	5 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypercalcic Mesonatric Brown Sodosol     	Principal Profile Form:	Db1.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.06 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Clay loam, sandy; Massive grade of structure; Moist; 10-20%, 
	fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Field pH 6.5 (Raupach); Abrupt, Wavy change 
	to - 
	B21	0.06 - 0.25 m	Strong brown (7.5YR4/6-Moist); Mechanical, 7.5YR32, 10-20% , 15-30mm, Distinct; Sandy medium clay;
	 Moderate grade of structure; Rough-ped fabric; Moderately moist; Soil matrix is Slightly calcareous; 
	Field pH 8.5 (Raupach); Clear change to - 
	B22k	0.25 - 0.4 m	Strong brown (7.5YR4/6-Moist); , 0-0% ; Sandy medium clay; Moderate grade of structure; Rough-ped 
	fabric; Moderately moist; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; Soil 
	matrix is Moderately calcareous; Field pH 9 (Raupach); Clear change to - 
	B23k	0.4 - 0.6 m	Brown (7.5YR5/4-Moist); , 0-0% ; Medium clay; Moderate grade of structure; Rough-ped fabric; 
	Moderately moist; 20-50%, medium gravelly, 6-20mm, subangular, Calcrete, coarse fragments; Many (20
	 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; Soil matrix is Moderately calcareous; 
	Field pH 9 (Raupach); 
	Morphological Notes
	B21	Cutans.         
	B23k	Duplicated "common" carbonate "nodules" removed from segregations table
	Observation Notes
	Site Notes
	"Hardsetting grey clay".    ESP=15, just Mesonatric

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0327	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	5.9B	14B	4.22A	4.56	0.61	0.65	10.04D
	6.7H
	0 - 0.06	5.9B	14B	4.22A	4.56	0.61	0.65	10.04D
	6.7H
	0 - 0.06	5.9B	14B	4.22A	4.56	0.61	0.65	10.04D
	6.7H
	0.06 - 0.25	8.3B	31B	5.13E	9.6	0.65	2.56	17B	17.94D	15.06
	9.2H
	0.06 - 0.25	8.3B	31B	5.13E	9.6	0.65	2.56	17B	17.94D	15.06
	9.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	1.75D	76.5I	6	17.5
	0 - 0.06	1.75D	76.5I	6	17.5
	0 - 0.06	1.75D	76.5I	6	17.5
	0.06 - 0.25	5C	0.3D	56I	5	39
	0.06 - 0.25	5C	0.3D	56I	5	39
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0327	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded