Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0343	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	03/08/95	Elevation:	270 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6247890 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	595070  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	10 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition 	Cracking, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epihypersodic Pedal Calcic Calcarosol     	Principal Profile Form:	Ug6.6
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	; 10-20%, , subangular, Gabbro
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish brown (5YR3/2-Moist); , 0-0% ; Light clay; Weak grade of structure, Subangular blocky; 
	Rough-ped fabric; Moist; Weak consistence; Soil matrix is Slightly calcareous; Field pH 8.5 (Raupach); 
	Abrupt, Wavy change to - 
	B21	0.05 - 0.4 m	Reddish brown (5YR4/4-Moist); Mechanical, 5YR32, 10-20% , 5-15mm, Faint; Medium clay; Strong 
	grade of structure; Rough-ped fabric; Moist; Firm consistence; Few cutans, <10% of ped faces or walls 
	coated; Soil matrix is Moderately calcareous; Field pH 8.5 (Raupach); Clear change to - 
	B22k	0.4 - 0.7 m	Reddish brown (5YR4/4-Moist); Mechanical, 5YR32, 2-10% , 0-5mm, Faint; Medium clay; Strong grade 
	of structure; Smooth-ped fabric; Dry; Very firm consistence; Few cutans, <10% of ped faces or walls 
	coated; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; Soil matrix is Highly 
	calcareous; Field pH 9 (Raupach); 
	Morphological Notes
	B21	Cutans 5YR 3/2, few slickensides.         
	B22k	Cutans 5YR 3/2, few slickensides.         
	Observation Notes
	Site Notes
	Site along Jackitup Road.    

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0343	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.2B	22B	23.26A	7.11	1.62	0.7	32.69D
	7.8H
	6.8B
	0 - 0.05	7.2B	22B	23.26A	7.11	1.62	0.7	32.69D
	7.8H
	6.8B
	0 - 0.05	7.2B	22B	23.26A	7.11	1.62	0.7	32.69D
	7.8H
	6.8B
	0.05 - 0.25	8.1B	23B	22.8E	13.61	0.81	3.62	38B	40.84D	9.53
	9H
	0.05 - 0.25	8.1B	23B	22.8E	13.61	0.81	3.62	38B	40.84D	9.53
	9H
	0.15 - 0.25	8B
	0.4 - 0.5	8.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	2.44D	57I	13.5	29.5
	0 - 0.05	2.44D	57I	13.5	29.5
	0 - 0.05	2.44D	57I	13.5	29.5
	0.05 - 0.25	4C	0.96D	38.5I
	0.05 - 0.25	4C	0.96D	38.5I
	0.15 - 0.25
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0343	Observation 	1
	Agency Name:	Agriculture Western Australia
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P10_NR_ZC	Silt + clay (%) - Not recorded