Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0361	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	07/08/95	Elevation:	290 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6242915 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	606240  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	10 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	270 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Hypernatric Grey Sodosol     	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	20-50%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , subangular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sand; Massive grade of structure; Moist; Field pH 5.5 (Raupach); 
	Sharp, Smooth change to - 
	A2e	0.1 - 0.15 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Moist; Field pH 
	6 (Raupach); Abrupt, Irregular change to - 
	B21	0.15 - 0.4 m	Light brownish grey (10YR6/2-Moist); Mottles, 2.5YR46, 10-20% , 15-30mm, Distinct; Sandy medium 
	clay; Moderate grade of structure, Columnar; Rough-ped fabric; Moderately moist; Firm consistence; 
	Field pH 7.5 (Raupach); Gradual change to - 
	B22	0.4 - 0.6 m	Light brownish grey (2.5Y6/2-Moist); Mottles, 2.5YR46, 2-10% , 5-15mm, Distinct; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Dry; Very firm consistence; Field pH 6 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0361	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.6B	10B	2.16H	0.39	0.1	0.16	0.25J	2.81D
	5.5H
	4.4B
	0 - 0.1	4.6B	10B	2.16H	0.39	0.1	0.16	0.25J	2.81D
	5.5H
	4.4B
	0 - 0.1	4.6B	10B	2.16H	0.39	0.1	0.16	0.25J	2.81D
	5.5H
	4.4B
	0 - 0.1	4.6B	10B	2.16H	0.39	0.1	0.16	0.25J	2.81D
	5.5H
	4.4B
	0.15 - 0.35	6.3B	19B	2.37A	4.68	0.06	2.15	9.26D
	7.4H
	0.15 - 0.35	6.3B	19B	2.37A	4.68	0.06	2.15	9.26D
	7.4H
	0.15 - 0.35	6.3B	19B	2.37A	4.68	0.06	2.15	9.26D
	7.4H
	0.15 - 0.25	6.3B
	0.4 - 0.5	5.9B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.3D	90I	5	5
	0 - 0.1	1.3D	90I	5	5
	0 - 0.1	1.3D	90I	5	5
	0 - 0.1	1.3D	90I	5	5
	0.15 - 0.35	0.25D	53I	5	42
	0.15 - 0.35	0.25D	53I	5	42
	0.15 - 0.35	0.25D	53I	5	42
	0.15 - 0.25
	0.4 - 0.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0361	Observation 	1
	Agency Name:	Agriculture Western Australia
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded