Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0398	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	29/08/95	Elevation:	270 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6240900 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	629500  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	5 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Mesonatric Yellow Sodosol     	Principal Profile Form:	Dy2.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	20-50%, medium gravelly, 6-20mm, subrounded, ; 10-20%, , subangular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-0% ; Clayey sand; Massive grade of structure; 20-50%, 
	medium gravelly, 6-20mm, subangular, , coarse fragments; 10-20%, medium gravelly, 6-20mm, 
	subrounded, Quartz, coarse fragments; Field pH 6 (Raupach); Abrupt, Smooth change to - 
	A3	0.1 - 0.12 m	Brown (10YR5/3-Moist); , 0-0% ; Clayey sand; Massive grade of structure; 10-20%, fine gravelly, 2-6mm,
	 subangular, Quartz, coarse fragments; Field pH 6.5 (Raupach); Abrupt, Wavy change to - 
	B21	0.12 - 0.4 m	Brownish yellow (10YR6/6-Moist); , 0-0% ; Medium clay; Moderate grade of structure; Rough-ped fabric;
	 Dry; 0-2%, fine gravelly, 2-6mm, Calcrete, coarse fragments; Soil matrix is Slightly calcareous; Field pH
	 9 (Raupach); Gradual change to - 
	B22	0.4 - 0.5 m	Olive yellow (2.5Y6/6-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; Rough-ped fabric;
	 Dry; 0-2%, fine gravelly, 2-6mm, Calcrete, coarse fragments; Soil matrix is Slightly calcareous; Field pH
	 9.5 (Raupach); 
	Morphological Notes
	B22	Stopped by large carbonate nodule.         
	Observation Notes
	Site Notes
	Site in lupin crop - drainage line downslope is affected by severe salinity and moderate sheet and rill erosion - "hardsetting grey clay".

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0398	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9B	6B	3.06H	0.63	0.22	0.04	0.11J	3.95D
	5.8H
	0 - 0.1	4.9B	6B	3.06H	0.63	0.22	0.04	0.11J	3.95D
	5.8H
	0 - 0.1	4.9B	6B	3.06H	0.63	0.22	0.04	0.11J	3.95D
	5.8H
	0.12 - 0.32	8.3B	21B	4E	4.56	0.74	0.84	11B	10.14D	7.64
	9.1H
	0.12 - 0.32	8.3B	21B	4E	4.56	0.74	0.84	11B	10.14D	7.64
	9.1H
	0.12 - 0.32	8.3B	21B	4E	4.56	0.74	0.84	11B	10.14D	7.64
	9.1H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.16D	90I	4.5	5.5
	0 - 0.1	1.16D	90I	4.5	5.5
	0 - 0.1	1.16D	90I	4.5	5.5
	0.12 - 0.32	<2C	0.2D	55.5I	3.5	41
	0.12 - 0.32	<2C	0.2D	55.5I	3.5	41
	0.12 - 0.32	<2C	0.2D	55.5I	3.5	41
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0398	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded