Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0411	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	30/08/95	Elevation:	270 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6242550 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	636450  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	5 metres
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	1 % 	Aspect:	90 degrees
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Mesonatric Yellow Sodosol     	Principal Profile Form:	Dy2.12
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, angular, Quartz; 2-10%, , subangular, Quartz
	Profile Morphology
	Ap	0 - 0.08 m	Dark grey (10YR4/1-Moist); , 0-0% ; Sandy loam; Massive grade of structure; Dry; Field pH 6.5 
	(Raupach); Abrupt, Wavy change to - 
	B21	0.08 - 0.35 m	Light yellowish brown (2.5Y6/4-Moist); , 0-0% ; Sandy light medium clay; Weak grade of structure; 
	Rough-ped fabric; Dry; Field pH 7.5 (Raupach); Clear change to - 
	B22	0.35 - 0.55 m	Light brownish grey (2.5Y6/3-Moist); Mottles, 2.5YR46, 2-10% , 15-30mm, Distinct; Sandy medium clay; 
	Moderate grade of structure; Rough-ped fabric; Moderately moist; Very firm consistence; Soil matrix is 
	Slightly calcareous; Field pH 8.5 (Raupach); Abrupt change to - 
	B3	0.55 - 0.7 m	Yellowish red (5YR4/6-Moist); Mottles, 10YR58, 0-2% , 5-15mm, Distinct; Coarse sandy light medium 
	clay; Moderate grade of structure; Rough-ped fabric; Moderately moist; Very firm consistence; Field pH 
	7 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	 Some silcrete on surface at this site - "hardsetting grey clay".   Field texture was used to classify profile.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0411	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.7B	16B	5.29A	2.29	0.51	0.91	9D
	6.6H
	0 - 0.08	5.7B	16B	5.29A	2.29	0.51	0.91	9D
	6.6H
	0 - 0.08	5.7B	16B	5.29A	2.29	0.51	0.91	9D
	6.6H
	0.08 - 0.28	6.8B	21B	2.6A	3.96	0.33	1.5	8.39D
	7.9H
	0.08 - 0.28	6.8B	21B	2.6A	3.96	0.33	1.5	8.39D
	7.9H
	0.08 - 0.28	6.8B	21B	2.6A	3.96	0.33	1.5	8.39D
	7.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	1.74D	88.5I	7.5	12
	0 - 0.08	1.74D	88.5I	7.5	12
	0 - 0.08	1.74D	88.5I	7.5	12
	0.08 - 0.28	0.2D	71I	5.5	23.5
	0.08 - 0.28	0.2D	71I	5.5	23.5
	0.08 - 0.28	0.2D	71I	5.5	23.5
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded