Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0457	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Heather Percy	Locality:
	Date Desc.:	18/09/95	Elevation:	300 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6278580 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	634330  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	10 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting, Hardsetting
	Erosion	 (wind);  (sheet)  (rill)  (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mesonatric Grey Sodosol     	Principal Profile Form:	Dg2.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Loamy sand; Massive grade of structure; Dry; Field pH 6 
	(Raupach); Abrupt, Wavy change to - 
	B21k	0.1 - 0.3 m	Very pale brown (10YR7/3-Moist); , 0-0% ; Sandy medium clay; Moderate grade of structure; Rough-ped 
	fabric; Dry; Very firm consistence; 2-10%, fine gravelly, 2-6mm, Calcrete, coarse fragments; Few (2 - 10 
	%), Calcareous, Medium (2 -6 mm), Soft segregations; Soil matrix is Slightly calcareous; Field pH 8 
	(Raupach); Clear change to - 
	B22	0.3 - 0.6 m	Light grey (2.5Y7/2-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; Rough-ped fabric; 
	Moderately moist; Firm consistence; 2-10%, medium gravelly, 6-20mm, Calcrete, coarse fragments; Soil 
	matrix is Slightly calcareous; Field pH 9 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes
	"Hardsetting grey clay".

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0457	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.2B	5B	1.62A	1.25	0.24	0.22	3.33D
	6.6H
	0 - 0.1	5.2B	5B	1.62A	1.25	0.24	0.22	3.33D
	6.6H
	0 - 0.1	5.2B	5B	1.62A	1.25	0.24	0.22	3.33D
	6.6H
	0.1 - 0.3	8B	37B	2.7E	6.3	0.71	3.37	14B	13.08D	24.07
	9H
	0.1 - 0.3	8B	37B	2.7E	6.3	0.71	3.37	14B	13.08D	24.07
	9H
	0.1 - 0.3	8B	37B	2.7E	6.3	0.71	3.37	14B	13.08D	24.07
	9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.87D	89.5I	3.5	7
	0 - 0.1	0.87D	89.5I	3.5	7
	0 - 0.1	0.87D	89.5I	3.5	7
	0.1 - 0.3	<2C	0.29D	58.5I	3.5	38
	0.1 - 0.3	<2C	0.29D	58.5I	3.5	38
	0.1 - 0.3	<2C	0.29D	58.5I	3.5	38
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	0457	Observation 	1
	Agency Name:	Agriculture Western Australia
	4_NR	pH of soil - Not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded